#MicroXplorer Configuration settings - do not modify
ADC1.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_8
ADC1.ClockPrescaler=ADC_CLOCK_ASYNC_DIV1
ADC1.ContinuousConvMode=DISABLE
ADC1.DMAContinuousRequests=ENABLE
ADC1.DataAlign=ADC_DATAALIGN_RIGHT
ADC1.DiscontinuousConvMode=DISABLE
ADC1.EOCSelection=ADC_EOC_SINGLE_CONV
ADC1.EnableAnalogWatchDog1=false
ADC1.EnableAnalogWatchDog2=false
ADC1.EnableAnalogWatchDog3=false
ADC1.EnableInjectedConversion=DISABLE
ADC1.EnableRegularConversion=ENABLE
ADC1.ExternalTrigConv=ADC_EXTERNALTRIG_T6_TRGO
ADC1.ExternalTrigConvEdge=ADC_EXTERNALTRIGCONVEDGE_RISING
ADC1.IPParameters=Rank-0\#ChannelRegularConversion,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,OffsetNumber-0\#ChannelRegularConversion,NbrOfConversionFlag,DMAContinuousRequests,Overrun,ExternalTrigConv,OversamplingMode,ClockPrescaler,Resolution,DataAlign,ScanConvMode,ContinuousConvMode,DiscontinuousConvMode,EOCSelection,LowPowerAutoWait,EnableRegularConversion,NbrOfConversion,ExternalTrigConvEdge,EnableInjectedConversion,EnableAnalogWatchDog1,EnableAnalogWatchDog2,EnableAnalogWatchDog3,RightBitShift,Ratio,OversamplingStopReset,TriggeredMode,master
ADC1.LowPowerAutoWait=DISABLE
ADC1.NbrOfConversion=1
ADC1.NbrOfConversionFlag=1
ADC1.OffsetNumber-0\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.Overrun=ADC_OVR_DATA_OVERWRITTEN
ADC1.OversamplingMode=ENABLE
ADC1.OversamplingStopReset=ADC_REGOVERSAMPLING_CONTINUED_MODE
ADC1.Rank-0\#ChannelRegularConversion=1
ADC1.Ratio=ADC_OVERSAMPLING_RATIO_16
ADC1.Resolution=ADC_RESOLUTION_12B
ADC1.RightBitShift=ADC_RIGHTBITSHIFT_2
ADC1.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_6CYCLES_5
ADC1.ScanConvMode=ADC_SCAN_DISABLE
ADC1.TriggeredMode=ADC_TRIGGEREDMODE_SINGLE_TRIGGER
ADC1.master=1
CRC.CRCLength=CRC_POLYLENGTH_16B
CRC.DefaultInitValueUse=DEFAULT_INIT_VALUE_DISABLE
CRC.DefaultPolynomialUse=DEFAULT_POLYNOMIAL_DISABLE
CRC.GeneratingPolynomial=X12+X5+X0
CRC.IPParameters=DefaultPolynomialUse,CRCLength,GeneratingPolynomial,DefaultInitValueUse,InitValue,InputDataInversionMode
CRC.InitValue=0xFFFF
CRC.InputDataInversionMode=CRC_INPUTDATA_INVERSION_BYTE
DAC1.DAC_Channel-DAC_OUT2=DAC_CHANNEL_2
DAC1.DAC_Trigger-DAC_OUT1=DAC_TRIGGER_T7_TRGO
DAC1.IPParameters=DAC_Channel-DAC_OUT2,DAC_Trigger-DAC_OUT1
Dma.ADC1.3.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC1.3.Instance=DMA1_Channel1
Dma.ADC1.3.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC1.3.MemInc=DMA_MINC_ENABLE
Dma.ADC1.3.Mode=DMA_CIRCULAR
Dma.ADC1.3.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC1.3.PeriphInc=DMA_PINC_DISABLE
Dma.ADC1.3.Priority=DMA_PRIORITY_LOW
Dma.ADC1.3.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority
Dma.DAC_CH1.2.Direction=DMA_MEMORY_TO_PERIPH
Dma.DAC_CH1.2.Instance=DMA2_Channel4
Dma.DAC_CH1.2.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.DAC_CH1.2.MemInc=DMA_MINC_ENABLE
Dma.DAC_CH1.2.Mode=DMA_CIRCULAR
Dma.DAC_CH1.2.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.DAC_CH1.2.PeriphInc=DMA_PINC_DISABLE
Dma.DAC_CH1.2.Priority=DMA_PRIORITY_LOW
Dma.DAC_CH1.2.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority
Dma.I2C3_RX.4.Direction=DMA_PERIPH_TO_MEMORY
Dma.I2C3_RX.4.Instance=DMA1_Channel3
Dma.I2C3_RX.4.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.I2C3_RX.4.MemInc=DMA_MINC_ENABLE
Dma.I2C3_RX.4.Mode=DMA_NORMAL
Dma.I2C3_RX.4.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.I2C3_RX.4.PeriphInc=DMA_PINC_DISABLE
Dma.I2C3_RX.4.Priority=DMA_PRIORITY_LOW
Dma.I2C3_RX.4.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority
Dma.I2C3_TX.5.Direction=DMA_MEMORY_TO_PERIPH
Dma.I2C3_TX.5.Instance=DMA1_Channel2
Dma.I2C3_TX.5.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.I2C3_TX.5.MemInc=DMA_MINC_ENABLE
Dma.I2C3_TX.5.Mode=DMA_NORMAL
Dma.I2C3_TX.5.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.I2C3_TX.5.PeriphInc=DMA_PINC_DISABLE
Dma.I2C3_TX.5.Priority=DMA_PRIORITY_LOW
Dma.I2C3_TX.5.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority
Dma.Request0=USART2_RX
Dma.Request1=USART2_TX
Dma.Request2=DAC_CH1
Dma.Request3=ADC1
Dma.Request4=I2C3_RX
Dma.Request5=I2C3_TX
Dma.RequestsNb=6
Dma.USART2_RX.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.USART2_RX.0.Instance=DMA1_Channel6
Dma.USART2_RX.0.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART2_RX.0.MemInc=DMA_MINC_ENABLE
Dma.USART2_RX.0.Mode=DMA_NORMAL
Dma.USART2_RX.0.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART2_RX.0.PeriphInc=DMA_PINC_DISABLE
Dma.USART2_RX.0.Priority=DMA_PRIORITY_LOW
Dma.USART2_RX.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority
Dma.USART2_TX.1.Direction=DMA_MEMORY_TO_PERIPH
Dma.USART2_TX.1.Instance=DMA1_Channel7
Dma.USART2_TX.1.MemDataAlignment=DMA_MDATAALIGN_BYTE
Dma.USART2_TX.1.MemInc=DMA_MINC_ENABLE
Dma.USART2_TX.1.Mode=DMA_NORMAL
Dma.USART2_TX.1.PeriphDataAlignment=DMA_PDATAALIGN_BYTE
Dma.USART2_TX.1.PeriphInc=DMA_PINC_DISABLE
Dma.USART2_TX.1.Priority=DMA_PRIORITY_LOW
Dma.USART2_TX.1.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority
FREERTOS.FootprintOK=true
FREERTOS.HEAP_NUMBER=4
FREERTOS.IPParameters=Tasks01,FootprintOK,configUSE_TICKLESS_IDLE,MEMORY_ALLOCATION,configTOTAL_HEAP_SIZE,HEAP_NUMBER,configUSE_TIMERS,Queues01,Timers01,configCHECK_FOR_STACK_OVERFLOW
FREERTOS.MEMORY_ALLOCATION=2
FREERTOS.Queues01=ioEventQueue,16,uint32_t,0,Static,ioEventQueueBuffer,ioEventQueueControlBlock;serialInputQueue,16,uint32_t,0,Static,serialInputQueueBuffer,serialInputQueueControlBlock;serialOutputQueue,16,uint32_t,0,Static,serialOutputQueueBuffer,serialOutputQueueControlBlock;audioInputQueue,4,uint8_t,0,Static,audioInputQueueBuffer,audioInputQueueControlBlock;hdlcInputQueue,3,uint32_t,0,Static,hdlcInputQueueBuffer,hdlcInputQueueControlBlock;hdlcOutputQueue,3,uint32_t,0,Static,hdlcOutputQueueBuffer,hdlcOutputQueueControlBlock;dacOutputQueue,128,uint8_t,0,Static,dacOutputQueueBuffer,dacOutputQueueControlBlock;adcInputQueue,3,uint32_t,0,Static,adcInputQueueBuffer,adcInputQueueControlBlock
FREERTOS.Tasks01=defaultTask,-3,256,startDefaultTask,Default,NULL,Static,defaultTaskBuffer,defaultTaskControlBlock;ioEventTask,-2,384,startIOEventTask,As external,NULL,Static,ioEventTaskBuffer,ioEventTaskControlBlock;audioInputTask,0,512,startAudioInputTask,As external,NULL,Static,audioInputTaskBuffer,audioInputTaskControlBlock;modulatorTask,0,384,startModulatorTask,As external,NULL,Static,modulatorTaskBuffer,modulatorTaskControlBlock
FREERTOS.Timers01=beaconTimer1,onBeaconTimer1,osTimerPeriodic,As external,NULL,Dynamic,NULL;beaconTimer2,onBeaconTimer2,osTimerPeriodic,As external,NULL,Dynamic,NULL;beaconTimer3,onBeaconTimer3,osTimerPeriodic,As external,NULL,Dynamic,NULL;beaconTimer4,onBeaconTimer4,osTimerPeriodic,As external,NULL,Dynamic,NULL
FREERTOS.configCHECK_FOR_STACK_OVERFLOW=2
FREERTOS.configTOTAL_HEAP_SIZE=4096
FREERTOS.configUSE_TICKLESS_IDLE=1
FREERTOS.configUSE_TIMERS=1
File.Version=6
I2C3.I2C_Speed_Mode=I2C_Fast
I2C3.IPParameters=Timing,I2C_Speed_Mode
I2C3.Timing=0x2010091A
KeepUserPlacement=true
Mcu.Family=STM32L4
Mcu.IP0=ADC1
Mcu.IP1=CRC
Mcu.IP10=SYS
Mcu.IP11=TIM6
Mcu.IP12=TIM7
Mcu.IP13=USART2
Mcu.IP2=DAC1
Mcu.IP3=DMA
Mcu.IP4=FREERTOS
Mcu.IP5=I2C3
Mcu.IP6=NVIC
Mcu.IP7=OPAMP1
Mcu.IP8=RCC
Mcu.IP9=RTC
Mcu.IPNb=14
Mcu.Name=STM32L432K(B-C)Ux
Mcu.Package=UFQFPN32
Mcu.Pin0=PC14-OSC32_IN (PC14)
Mcu.Pin1=PC15-OSC32_OUT (PC15)
Mcu.Pin10=PA8
Mcu.Pin11=PA9
Mcu.Pin12=PA10
Mcu.Pin13=PA11
Mcu.Pin14=PA12
Mcu.Pin15=PA13 (JTMS-SWDIO)
Mcu.Pin16=PA14 (JTCK-SWCLK)
Mcu.Pin17=PA15 (JTDI)
Mcu.Pin18=PB3 (JTDO-TRACESWO)
Mcu.Pin19=PB4 (NJTRST)
Mcu.Pin2=PA0
Mcu.Pin20=PB5
Mcu.Pin21=PB6
Mcu.Pin22=PB7
Mcu.Pin23=VP_ADC1_OPAMP1_OUT
Mcu.Pin24=VP_CRC_VS_CRC
Mcu.Pin25=VP_FREERTOS_VS_ENABLE
Mcu.Pin26=VP_RTC_VS_RTC_Activate
Mcu.Pin27=VP_RTC_VS_RTC_Calendar
Mcu.Pin28=VP_SYS_VS_tim2
Mcu.Pin29=VP_TIM6_VS_ClockSourceINT
Mcu.Pin3=PA1
Mcu.Pin30=VP_TIM7_VS_ClockSourceINT
Mcu.Pin4=PA2
Mcu.Pin5=PA3
Mcu.Pin6=PA4
Mcu.Pin7=PA5
Mcu.Pin8=PA7
Mcu.Pin9=PB1
Mcu.PinsNb=31
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32L432KCUx
MxCube.Version=4.27.0
MxDb.Version=DB.4.0.270
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:false\:false\:false
NVIC.DMA1_Channel1_IRQn=true\:5\:0\:false\:false\:true\:true\:false
NVIC.DMA1_Channel2_IRQn=true\:5\:0\:false\:false\:true\:true\:false
NVIC.DMA1_Channel3_IRQn=true\:5\:0\:false\:false\:true\:true\:false
NVIC.DMA1_Channel6_IRQn=true\:5\:0\:false\:false\:true\:true\:false
NVIC.DMA1_Channel7_IRQn=true\:5\:0\:false\:false\:true\:true\:false
NVIC.DMA2_Channel4_IRQn=true\:5\:0\:false\:false\:true\:true\:false
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:false\:false\:false
NVIC.EXTI1_IRQn=true\:5\:0\:false\:false\:true\:true\:true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:false\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:false\:false\:false
NVIC.PendSV_IRQn=true\:15\:0\:false\:false\:false\:true\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:false\:false\:false
NVIC.SysTick_IRQn=true\:15\:0\:true\:false\:true\:true\:true
NVIC.TIM2_IRQn=true\:0\:0\:false\:false\:true\:false\:false
NVIC.TimeBase=TIM2_IRQn
NVIC.TimeBaseIP=TIM2
NVIC.USART2_IRQn=true\:6\:0\:true\:false\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:false\:false\:false
OPAMP1.IPParameters=PowerSupplyRange
OPAMP1.PowerSupplyRange=OPAMP_POWERSUPPLY_HIGH
PA0.Locked=true
PA0.Mode=PGA Connected
PA0.Signal=OPAMP1_VINP
PA1.Locked=true
PA1.Mode=PGA Connected
PA1.Signal=OPAMP1_VINM
PA10.GPIOParameters=PinState,GPIO_Label,GPIO_ModeDefaultOutputPP
PA10.GPIO_Label=LED_YELLOW
PA10.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PA10.Locked=true
PA10.PinState=GPIO_PIN_SET
PA10.Signal=GPIO_Output
PA11.GPIOParameters=GPIO_Label
PA11.GPIO_Label=PTT_M
PA11.Locked=true
PA11.Signal=GPIO_Output
PA12.GPIOParameters=GPIO_Label
PA12.GPIO_Label=PTT_S
PA12.Locked=true
PA12.Signal=GPIO_Output
PA13\ (JTMS-SWDIO).GPIOParameters=GPIO_Label
PA13\ (JTMS-SWDIO).GPIO_Label=SWDIO
PA13\ (JTMS-SWDIO).Locked=true
PA13\ (JTMS-SWDIO).Mode=Serial_Wire
PA13\ (JTMS-SWDIO).Signal=SYS_JTMS-SWDIO
PA14\ (JTCK-SWCLK).GPIOParameters=GPIO_Label
PA14\ (JTCK-SWCLK).GPIO_Label=SWCLK
PA14\ (JTCK-SWCLK).Locked=true
PA14\ (JTCK-SWCLK).Mode=Serial_Wire
PA14\ (JTCK-SWCLK).Signal=SYS_JTCK-SWCLK
PA15\ (JTDI).GPIOParameters=GPIO_Label
PA15\ (JTDI).GPIO_Label=VCP_RX
PA15\ (JTDI).Locked=true
PA15\ (JTDI).Mode=Asynchronous
PA15\ (JTDI).Signal=USART2_RX
PA2.GPIOParameters=GPIO_Label
PA2.GPIO_Label=VCP_TX
PA2.Locked=true
PA2.Mode=Asynchronous
PA2.Signal=USART2_TX
PA3.GPIOParameters=GPIO_Label
PA3.GPIO_Label=AUDIO_IN
PA3.Locked=true
PA3.Signal=SharedAnalog_PA3
PA4.GPIOParameters=GPIO_Label
PA4.GPIO_Label=AUDIO_OUT_DAC
PA4.Locked=true
PA4.Signal=COMP_DAC11_group
PA5.GPIOParameters=GPIO_Label
PA5.GPIO_Label=AUDIO_IN_VREF
PA5.Locked=true
PA5.Signal=COMP_DAC12_group
PA7.GPIOParameters=GPIO_PuPdOD
PA7.GPIO_PuPdOD=GPIO_NOPULL
PA7.Locked=true
PA7.Mode=I2C
PA7.Signal=I2C3_SCL
PA8.GPIOParameters=PinState,GPIO_Label,GPIO_ModeDefaultOutputPP
PA8.GPIO_Label=LED_RED
PA8.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PA8.Locked=true
PA8.PinState=GPIO_PIN_SET
PA8.Signal=GPIO_Output
PA9.GPIOParameters=PinState,GPIO_Label,GPIO_ModeDefaultOutputPP
PA9.GPIO_Label=LED_GREEN
PA9.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PA9.Locked=true
PA9.PinState=GPIO_PIN_SET
PA9.Signal=GPIO_Output
PB1.GPIOParameters=GPIO_PuPd,GPIO_Label,GPIO_ModeDefaultEXTI
PB1.GPIO_Label=BUTTON_AUDIO_IN_ADJUST
PB1.GPIO_ModeDefaultEXTI=GPIO_MODE_IT_FALLING
PB1.GPIO_PuPd=GPIO_PULLUP
PB1.Locked=true
PB1.Signal=GPXTI1
PB3\ (JTDO-TRACESWO).GPIOParameters=GPIO_Label
PB3\ (JTDO-TRACESWO).GPIO_Label=LD3 [Green]
PB3\ (JTDO-TRACESWO).Locked=true
PB3\ (JTDO-TRACESWO).Signal=GPIO_Output
PB4\ (NJTRST).GPIOParameters=GPIO_PuPdOD
PB4\ (NJTRST).GPIO_PuPdOD=GPIO_NOPULL
PB4\ (NJTRST).Locked=true
PB4\ (NJTRST).Mode=I2C
PB4\ (NJTRST).Signal=I2C3_SDA
PB5.GPIOParameters=PinState,GPIO_Label,GPIO_ModeDefaultOutputPP
PB5.GPIO_Label=AUDIO_OUT_ATTEN
PB5.GPIO_ModeDefaultOutputPP=GPIO_MODE_OUTPUT_OD
PB5.Locked=true
PB5.PinState=GPIO_PIN_SET
PB5.Signal=GPIO_Output
PB6.Locked=true
PB6.Signal=GPIO_Analog
PB7.Locked=true
PB7.Signal=GPIO_Analog
PC14-OSC32_IN\ (PC14).Locked=true
PC14-OSC32_IN\ (PC14).Mode=LSE-External-Oscillator
PC14-OSC32_IN\ (PC14).Signal=RCC_OSC32_IN
PC15-OSC32_OUT\ (PC15).Locked=true
PC15-OSC32_OUT\ (PC15).Mode=LSE-External-Oscillator
PC15-OSC32_OUT\ (PC15).Signal=RCC_OSC32_OUT
PCC.Checker=true
PCC.Line=STM32L4x2
PCC.MCU=STM32L432K(B-C)Ux
PCC.PartNumber=STM32L432KCUx
PCC.Seq0=0
PCC.Series=STM32L4
PCC.Temperature=25
PCC.Vdd=null
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerOptimize=3
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32L432KCUx
ProjectManager.FirmwarePackage=STM32Cube FW_L4 V1.12.0
ProjectManager.FreePins=true
ProjectManager.HalAssertFull=true
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=true
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=TrueSTUDIO
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=Nucleo_L432KC_TNC.ioc
ProjectManager.ProjectName=Nucleo_L432KC_TNC
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=TrueSTUDIO
ProjectManager.ToolChainLocation=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-MX_GPIO_Init-GPIO-false-HAL-true,2-MX_DMA_Init-DMA-false-HAL-true,3-SystemClock_Config-RCC-false-HAL-false,4-MX_ADC1_Init-ADC1-false-HAL-true,5-MX_CRC_Init-CRC-false-HAL-true,6-MX_DAC1_Init-DAC1-false-HAL-true,7-MX_OPAMP1_Init-OPAMP1-false-HAL-true,8-MX_RTC_Init-RTC-false-HAL-true,9-MX_TIM6_Init-TIM6-false-HAL-true,10-MX_TIM7_Init-TIM7-false-HAL-true,11-MX_USART2_UART_Init-USART2-false-HAL-true,12-MX_I2C3_Init-I2C3-false-HAL-true
RCC.48CLKFreq_Value=24000000
RCC.ADCFreq_Value=80000000
RCC.AHBFreq_Value=48000000
RCC.APB1Freq_Value=48000000
RCC.APB1TimFreq_Value=48000000
RCC.APB2Freq_Value=48000000
RCC.APB2TimFreq_Value=48000000
RCC.CortexFreq_Value=48000000
RCC.FCLKCortexFreq_Value=48000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=48000000
RCC.HSE_VALUE=8000000
RCC.HSI16_VALUE=16000000
RCC.HSI48_VALUE=48000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=48000000
RCC.I2C2Freq_Value=16000000
RCC.I2C3Freq_Value=48000000
RCC.IPParameters=48CLKFreq_Value,ADCFreq_Value,AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,CortexFreq_Value,FCLKCortexFreq_Value,FamilyName,HCLKFreq_Value,HSE_VALUE,HSI16_VALUE,HSI48_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,LCDFreq_Value,LPTIM1Freq_Value,LPTIM2Freq_Value,LPTIMFreq_Value,LPUART1Freq_Value,LPUARTFreq_Value,LSCOPinFreq_Value,LSI_VALUE,MCO1PinFreq_Value,MCOPinFreq_Value,MSI_VALUE,PLLCLKFreq_Value,PLLMUL,PLLN,PLLPoutputFreq_Value,PLLQoutputFreq_Value,PLLRCLKFreq_Value,PLLSAI1N,PLLSAI1PoutputFreq_Value,PLLSAI1QoutputFreq_Value,PLLSAI1RoutputFreq_Value,PREFETCH_ENABLE,PWRFreq_Value,RNGFreq_Value,RTCClockSelection,RTCFreq_Value,RTCHSEDivFreq_Value,SAI1Freq_Value,SWPMI1Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,TIMFreq_Value,TimerFreq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USBFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value,VCOSAI1OutputFreq_Value,WatchDogFreq_Value
RCC.LCDFreq_Value=37000
RCC.LPTIM1Freq_Value=48000000
RCC.LPTIM2Freq_Value=48000000
RCC.LPTIMFreq_Value=32000000
RCC.LPUART1Freq_Value=48000000
RCC.LPUARTFreq_Value=32000000
RCC.LSCOPinFreq_Value=32000
RCC.LSI_VALUE=32000
RCC.MCO1PinFreq_Value=48000000
RCC.MCOPinFreq_Value=32000000
RCC.MSI_VALUE=4000000
RCC.PLLCLKFreq_Value=32000000
RCC.PLLMUL=RCC_PLLMUL_4
RCC.PLLN=24
RCC.PLLPoutputFreq_Value=13714285.714285715
RCC.PLLQoutputFreq_Value=48000000
RCC.PLLRCLKFreq_Value=48000000
RCC.PLLSAI1N=40
RCC.PLLSAI1PoutputFreq_Value=22857142.85714286
RCC.PLLSAI1QoutputFreq_Value=80000000
RCC.PLLSAI1RoutputFreq_Value=80000000
RCC.PREFETCH_ENABLE=1
RCC.PWRFreq_Value=48000000
RCC.RNGFreq_Value=80000000
RCC.RTCClockSelection=RCC_RTCCLKSOURCE_LSE
RCC.RTCFreq_Value=32768
RCC.RTCHSEDivFreq_Value=4000000
RCC.SAI1Freq_Value=22857142.85714286
RCC.SWPMI1Freq_Value=48000000
RCC.SYSCLKFreq_VALUE=48000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.TIMFreq_Value=32000000
RCC.TimerFreq_Value=32000000
RCC.USART1Freq_Value=48000000
RCC.USART2Freq_Value=48000000
RCC.USART3Freq_Value=16000000
RCC.USBFreq_Value=80000000
RCC.VCOInputFreq_Value=4000000
RCC.VCOOutputFreq_Value=96000000
RCC.VCOSAI1OutputFreq_Value=160000000
RCC.WatchDogFreq_Value=32000
SH.COMP_DAC11_group.0=DAC1_OUT1,DAC_OUT1
SH.COMP_DAC11_group.ConfNb=1
SH.COMP_DAC12_group.0=DAC1_OUT2,DAC_OUT2
SH.COMP_DAC12_group.ConfNb=1
SH.GPXTI1.0=GPIO_EXTI1
SH.GPXTI1.ConfNb=1
SH.SharedAnalog_PA3.0=ADC1_IN8
SH.SharedAnalog_PA3.1=OPAMP1_VOUT,PGA Connected
SH.SharedAnalog_PA3.ConfNb=2
TIM6.AutoReloadPreload=TIM_AUTORELOAD_PRELOAD_DISABLE
TIM6.IPParameters=Period,AutoReloadPreload,TIM_MasterOutputTrigger
TIM6.Period=1817
TIM6.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
TIM7.IPParameters=Period,TIM_MasterOutputTrigger
TIM7.Period=1817
TIM7.TIM_MasterOutputTrigger=TIM_TRGO_UPDATE
USART2.BaudRate=38400
USART2.IPParameters=VirtualMode-Asynchronous,BaudRate
USART2.VirtualMode-Asynchronous=VM_ASYNC
VP_ADC1_OPAMP1_OUT.Mode=IN8-OPAMP1-Single-Ended
VP_ADC1_OPAMP1_OUT.Signal=ADC1_OPAMP1_OUT
VP_CRC_VS_CRC.Mode=CRC_Activate
VP_CRC_VS_CRC.Signal=CRC_VS_CRC
VP_FREERTOS_VS_ENABLE.Mode=Enabled
VP_FREERTOS_VS_ENABLE.Signal=FREERTOS_VS_ENABLE
VP_RTC_VS_RTC_Activate.Mode=RTC_Enabled
VP_RTC_VS_RTC_Activate.Signal=RTC_VS_RTC_Activate
VP_RTC_VS_RTC_Calendar.Mode=RTC_Calendar
VP_RTC_VS_RTC_Calendar.Signal=RTC_VS_RTC_Calendar
VP_SYS_VS_tim2.Mode=TIM2
VP_SYS_VS_tim2.Signal=SYS_VS_tim2
VP_TIM6_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM6_VS_ClockSourceINT.Signal=TIM6_VS_ClockSourceINT
VP_TIM7_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM7_VS_ClockSourceINT.Signal=TIM7_VS_ClockSourceINT
board=NUCLEO-L432KC
boardIOC=true
