# RadioLib: src/modules/SX127x/SX1279.h Source File

SX1279.h
#if !defined(_RADIOLIB_SX1279_H)
#define _RADIOLIB_SX1279_H
#include "../../TypeDef.h"
#if !RADIOLIB_EXCLUDE_SX127X
#include "SX1278.h"
class SX1279: public SX1278 {
public:
// constructor
SX1279(Module* mod); // cppcheck-suppress noExplicitConstructor
// basic methods
int16_t begin(float freq = 434.0, float bw = 125.0, uint8_t sf = 9, uint8_t cr = 7, uint8_t syncWord = RADIOLIB_SX127X_SYNC_WORD, int8_t power = 10, uint16_t preambleLength = 8, uint8_t gain = 0);
int16_t beginFSK(float freq = 434.0, float br = 4.8, float freqDev = 5.0, float rxBw = 125.0, int8_t power = 10, uint16_t preambleLength = 16, bool enableOOK = false);
// configuration methods
int16_t setFrequency(float freq) override;
#if !RADIOLIB_GODMODE
private:
#endif
};
#endif
#endif
Module
Implements all common low-level methods to control the wireless module. Every module class contains o...
Definition: Module.h:68
SX1278
Derived class for SX1278 modules. Also used as base class for SX1276, SX1277, SX1279,...
Definition: SX1278.h:105
SX1279
Derived class for SX1279 modules. Overrides some methods from SX1278 due to different parameter range...
Definition: SX1279.h:14
SX1279::begin
int16_t begin(float freq=434.0, float bw=125.0, uint8_t sf=9, uint8_t cr=7, uint8_t syncWord=RADIOLIB_SX127X_SYNC_WORD, int8_t power=10, uint16_t preambleLength=8, uint8_t gain=0)
LoRa modem initialization method. Must be called at least once from Arduino sketch to initialize the ...
Definition: SX1279.cpp:8
SX1279::beginFSK
int16_t beginFSK(float freq=434.0, float br=4.8, float freqDev=5.0, float rxBw=125.0, int8_t power=10, uint16_t preambleLength=16, bool enableOOK=false)
FSK modem initialization method. Must be called at least once from Arduino sketch to initialize the m...
Definition: SX1279.cpp:40
SX1279::setFrequency
int16_t setFrequency(float freq) override
Sets carrier frequency. Allowed values range from 137.0 MHz to 960.0 MHz.
Definition: SX1279.cpp:71
SX1279::SX1279
SX1279(Module *mod)
Default constructor. Called from Arduino sketch when creating new LoRa instance.
Definition: SX1279.cpp:4