# RadioLib: Member List

SX1279 Member List

This is the complete list of members for SX1279, including all inherited members.

autoLDRO() | SX1278 |
available() | PhysicalLayer |
begin(float freq=434.0, float bw=125.0, uint8_t sf=9, uint8_t cr=7, uint8_t syncWord=RADIOLIB_SX127X_SYNC_WORD, int8_t power=10, uint16_t preambleLength=8, uint8_t gain=0) | SX1279 |
SX127x::begin(uint8_t *chipVersions, uint8_t numVersions, uint8_t syncWord, uint16_t preambleLength) | SX127x |
beginFSK(float freq=434.0, float br=4.8, float freqDev=5.0, float rxBw=125.0, int8_t power=10, uint16_t preambleLength=16, bool enableOOK=false) | SX1279 |
SX127x::beginFSK(uint8_t *chipVersions, uint8_t numVersions, float freqDev, float rxBw, uint16_t preambleLength, bool enableOOK) | SX127x |
calculateRxTimeout(RadioLibTime_t timeoutUs) override | SX127x | virtual
checkDataRate(DataRate_t dr) override | SX1278 | virtual
checkOutputPower(int8_t power, int8_t *clipped) override | SX1278 | virtual
checkOutputPower(int8_t power, int8_t *clipped, bool useRfo) | SX1278 |
clearChannelScanAction() override | SX127x | virtual
clearDio0Action() | SX127x |
clearDio1Action() | SX127x |
clearFHSSInt(void) | SX127x |
clearFifoEmptyAction() | SX127x |
clearFifoFullAction() | SX127x |
clearPacketReceivedAction() override | SX127x | virtual
clearPacketSentAction() override | SX127x | virtual
disableAddressFiltering() | SX127x |
disableBitSync() | SX127x |
dropSync() | PhysicalLayer |
enableBitSync() | SX127x |
explicitHeader() | SX1278 |
fifoAdd(uint8_t *data, int totalLen, int *remLen) | SX127x |
fifoGet(volatile uint8_t *data, int totalLen, volatile int *rcvLen) | SX127x |
finishTransmit() override | SX127x | virtual
fixedPacketLengthMode(uint8_t len=RADIOLIB_SX127X_MAX_PACKET_LENGTH_FSK) | SX127x |
forceLDRO(bool enable) | SX1278 |
getAFCError() | SX127x |
getChannelScanResult() override | SX127x | virtual
getChipVersion() | SX127x |
getDataRate() const | SX127x |
getFHSSChannel(void) | SX127x |
getFHSSHoppingPeriod(void) | SX127x |
getFreqStep() const | PhysicalLayer |
getFrequencyError(bool autoCorrect=false) | SX127x |
getIRQFlags() | SX127x |
getModemStatus() | SX127x |
getNumSymbols(size_t len) | SX127x |
getPacketLength(bool update=true) override | SX127x | virtual
getRSSI() override | SX1278 | virtual
getRSSI(bool packet, bool skipReceive=false) | SX1278 |
getSNR() override | SX127x | virtual
getTempRaw() | SX127x |
getTimeOnAir(size_t len) override | SX127x | virtual
implicitHeader(size_t len) | SX1278 |
invertIQ(bool enable) override | SX127x | virtual
invertPreamble(bool enable) | SX127x |
irqRxDoneRxTimeout(uint32_t &irqFlags, uint32_t &irqMask) override | SX127x | virtual
isRxTimeout() override | SX127x | virtual
packetMode() | SX127x |
PhysicalLayer(float step, size_t maxLen) | PhysicalLayer |
random(int32_t max) | PhysicalLayer |
random(int32_t min, int32_t max) | PhysicalLayer |
randomByte() override | SX127x | virtual
read(bool drop=true) | PhysicalLayer |
readBit(uint32_t pin) override | SX127x | virtual
readData(uint8_t *data, size_t len) override | SX127x | virtual
readData(uint8_t *data, size_t len) | SX127x |
receive(uint8_t *data, size_t len) override | SX127x | virtual
receive(uint8_t *data, size_t len) | SX127x |
receiveDirect() override | SX127x | virtual
reset() override | SX1278 | virtual
scanChannel() override | SX127x | virtual
setAFC(bool isEnabled) | SX127x |
setAFCAGCTrigger(uint8_t trigger) | SX127x |
setAFCBandwidth(float afcBw) | SX127x |
setBandwidth(float bw) | SX1278 |
setBitRate(float br) override | SX1278 | virtual
setBroadcastAddress(uint8_t broadAddr) | SX127x |
setChannelScanAction(void(*func)(void)) override | SX127x | virtual
setCodingRate(uint8_t cr) | SX1278 |
setCRC(bool enable, bool mode=false) | SX1278 |
setCrcFiltering(bool enable=true) | SX127x |
setCurrentLimit(uint8_t currentLimit) | SX127x |
setDataRate(DataRate_t dr) override | SX1278 | virtual
setDataShaping(uint8_t sh) override | SX1278 | virtual
setDataShapingOOK(uint8_t sh) | SX1278 |
setDio0Action(void(*func)(void), uint32_t dir) | SX127x |
setDio1Action(void(*func)(void), uint32_t dir) | SX127x |
setDIOMapping(uint32_t pin, uint32_t value) override | SX127x | virtual
setDIOPreambleDetect(bool usePreambleDetect) | SX127x |
setDirectAction(void(*func)(void)) override | SX127x | virtual
setDirectSyncWord(uint32_t syncWord, uint8_t len) | PhysicalLayer |
setEncoding(uint8_t encoding) override | SX127x | virtual
setFHSSHoppingPeriod(uint8_t freqHoppingPeriod) | SX127x |
setFifoEmptyAction(void(*func)(void)) | SX127x |
setFifoFullAction(void(*func)(void)) | SX127x |
setFrequency(float freq) override | SX1279 | virtual
setFrequencyDeviation(float freqDev) override | SX127x | virtual
setGain(uint8_t gain) | SX1278 |
setLowBatteryThreshold(int8_t level, uint32_t pin=RADIOLIB_NC) | SX127x |
setNodeAddress(uint8_t nodeAddr) | SX127x |
setOOK(bool enableOOK) | SX127x |
setOokFixedOrFloorThreshold(uint8_t value) | SX127x |
setOokPeakThresholdDecrement(uint8_t value) | SX127x |
setOokPeakThresholdStep(uint8_t value) | SX127x |
setOokThresholdType(uint8_t type) | SX127x |
setOutputPower(int8_t power) override | SX1278 | virtual
setOutputPower(int8_t power, bool useRfo) | SX1278 |
setPacketReceivedAction(void(*func)(void)) override | SX127x | virtual
setPacketSentAction(void(*func)(void)) override | SX127x | virtual
setPreambleLength(size_t preambleLength) override | SX127x | virtual
setRfSwitchPins(uint32_t rxEn, uint32_t txEn) | SX127x |
setRfSwitchTable(const uint32_t(&pins)[Module::RFSWITCH_MAX_PINS], const Module::RfSwitchMode_t table[]) | SX127x |
setRSSIConfig(uint8_t smoothingSamples, int8_t offset=0) | SX127x |
setRSSIThreshold(float dbm) | SX127x |
setRxBandwidth(float rxBw) | SX127x |
setSpreadingFactor(uint8_t sf) | SX1278 |
setSyncWord(uint8_t syncWord) | SX127x |
setSyncWord(uint8_t *syncWord, size_t len) override | SX127x | virtual
sleep() override | SX127x | virtual
standby() override | SX127x | virtual
standby(uint8_t mode) override | SX127x | virtual
startChannelScan() override | SX127x | virtual
startDirect() | PhysicalLayer |
startReceive() override | SX127x | virtual
startReceive(uint8_t len, uint8_t mode=RADIOLIB_SX127X_RXCONTINUOUS) | SX127x |
startReceive(uint32_t timeout, uint32_t irqFlags, uint32_t irqMask, size_t len) override | SX127x | virtual
startTransmit(uint8_t *data, size_t len, uint8_t addr=0) override | SX127x | virtual
startTransmit(const char *str, uint8_t addr=0) | SX127x |
startTransmit(uint8_t *data, size_t len, uint8_t addr=0) | SX127x |
PhysicalLayer::startTransmit(const char *str, uint8_t addr=0) | PhysicalLayer |
SX1278(Module *mod) | SX1278 |
SX1279(Module *mod) | SX1279 |
SX127x(Module *mod) | SX127x | explicit
transmit(uint8_t *data, size_t len, uint8_t addr=0) override | SX127x | virtual
transmit(const char *str, uint8_t addr=0) | SX127x |
transmit(uint8_t *data, size_t len, uint8_t addr=0) | SX127x |
PhysicalLayer::transmit(const char *str, uint8_t addr=0) | PhysicalLayer |
transmitDirect(uint32_t frf=0) override | SX127x | virtual
variablePacketLengthMode(uint8_t maxLen=RADIOLIB_SX127X_MAX_PACKET_LENGTH_FSK) | SX127x |