# RadioLib: Member List

LoRaWANNode Member List

This is the complete list of members for LoRaWANNode, including all inherited members.

beginABP(uint32_t addr, uint8_t *fNwkSIntKey, uint8_t *sNwkSIntKey, uint8_t *nwkSEncKey, uint8_t *appSKey, bool force=false, uint8_t initialDr=RADIOLIB_LW_DATA_RATE_UNUSED) | LoRaWANNode |
beginOTAA(uint64_t joinEUI, uint64_t devEUI, uint8_t *nwkKey, uint8_t *appKey, bool force=false, uint8_t joinDr=RADIOLIB_LW_DATA_RATE_UNUSED) | LoRaWANNode |
downlink(uint8_t *data, size_t *len, LoRaWANEvent_t *event=NULL) | LoRaWANNode |
downlink(LoRaWANEvent_t *event=NULL) | LoRaWANNode |
dutyCycleInterval(RadioLibTime_t msPerHour, RadioLibTime_t airtime) | LoRaWANNode |
getAFCntDown() | LoRaWANNode |
getBufferNonces() | LoRaWANNode |
getBufferSession() | LoRaWANNode |
getDevAddr() | LoRaWANNode |
getFCntUp() | LoRaWANNode |
getLastToA() | LoRaWANNode |
getMacDeviceTimeAns(uint32_t *gpsEpoch, uint8_t *fraction, bool returnUnix=true) | LoRaWANNode |
getMacLinkCheckAns(uint8_t *margin, uint8_t *gwCnt) | LoRaWANNode |
getNFCntDown() | LoRaWANNode |
isJoined() | LoRaWANNode |
LoRaWANNode(PhysicalLayer *phy, const LoRaWANBand_t *band, uint8_t subBand=0) | LoRaWANNode |
maxPayloadDwellTime() | LoRaWANNode |
resetFCntDown() | LoRaWANNode |
restore(uint16_t checkSum, uint16_t lwMode, uint8_t lwClass, uint8_t freqPlan) | LoRaWANNode |
rx1DrOffset | LoRaWANNode |
rx2 | LoRaWANNode |
saveSession() | LoRaWANNode |
sendMacCommandReq(uint8_t cid) | LoRaWANNode |
sendReceive(const char *strUp, uint8_t fPort, uint8_t *dataDown, size_t *lenDown, bool isConfirmed=false, LoRaWANEvent_t *eventUp=NULL, LoRaWANEvent_t *eventDown=NULL) | LoRaWANNode |
sendReceive(uint8_t *dataUp, size_t lenUp, uint8_t fPort, uint8_t *dataDown, size_t *lenDown, bool isConfirmed=false, LoRaWANEvent_t *eventUp=NULL, LoRaWANEvent_t *eventDown=NULL) | LoRaWANNode |
sendReceive(uint8_t *dataUp, size_t lenUp, uint8_t fPort=1, bool isConfirmed=false, LoRaWANEvent_t *eventUp=NULL, LoRaWANEvent_t *eventDown=NULL) | LoRaWANNode |
setADR(bool enable=true) | LoRaWANNode |
setBufferNonces(uint8_t *persistentBuffer) | LoRaWANNode |
setBufferSession(uint8_t *persistentBuffer) | LoRaWANNode |
setDatarate(uint8_t drUp) | LoRaWANNode |
setDeviceStatus(uint8_t battLevel) | LoRaWANNode |
setDutyCycle(bool enable=true, RadioLibTime_t msPerHour=0) | LoRaWANNode |
setDwellTime(bool enable, RadioLibTime_t msPerUplink=0) | LoRaWANNode |
setTxPower(int8_t txPower) | LoRaWANNode |
timeUntilUplink() | LoRaWANNode |
uplink(const char *str, uint8_t fPort, bool isConfirmed=false, LoRaWANEvent_t *event=NULL) | LoRaWANNode |
uplink(uint8_t *data, size_t len, uint8_t fPort, bool isConfirmed=false, LoRaWANEvent_t *event=NULL) | LoRaWANNode |
wipe() | LoRaWANNode |