# RadioLib: Member List

AX25Frame Member List

This is the complete list of members for AX25Frame, including all inherited members.

AX25Frame(const char *destCallsign, uint8_t destSSID, const char *srcCallsign, uint8_t srcSSID, uint8_t control) | AX25Frame |
AX25Frame(const char *destCallsign, uint8_t destSSID, const char *srcCallsign, uint8_t srcSSID, uint8_t control, uint8_t protocolID, const char *info) | AX25Frame |
AX25Frame(const char *destCallsign, uint8_t destSSID, const char *srcCallsign, uint8_t srcSSID, uint8_t control, uint8_t protocolID, uint8_t *info, uint16_t infoLen) | AX25Frame |
AX25Frame(const AX25Frame &frame) | AX25Frame |
control | AX25Frame |
destCallsign | AX25Frame |
destSSID | AX25Frame |
info | AX25Frame |
infoLen | AX25Frame |
numRepeaters | AX25Frame |
operator=(const AX25Frame &frame) | AX25Frame |
protocolID | AX25Frame |
rcvSeqNumber | AX25Frame |
repeaterCallsigns | AX25Frame |
repeaterSSIDs | AX25Frame |
sendSeqNumber | AX25Frame |
setRecvSequence(uint8_t seqNumber) | AX25Frame |
setRepeaters(char **repeaterCallsigns, uint8_t *repeaterSSIDs, uint8_t numRepeaters) | AX25Frame |
setSendSequence(uint8_t seqNumber) | AX25Frame |
srcCallsign | AX25Frame |
srcSSID | AX25Frame |
~AX25Frame() | AX25Frame |