(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "TTGO-T-Display" (in_bom yes) (on_board yes)
    (property "Reference" "MCU" (id 0) (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TTGO-T-Display" (id 1) (at 0 2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "TTGO_T_Display:TTGO-T-Display" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TTGO-T-Display_0_0"
      (text "BL_GPIO4" (at 1.27 -30.48 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "BTN_GPIO0" (at 21.59 -7.62 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "BTN_GPIO32" (at -19.05 -7.62 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "BTN_RST" (at -27.94 -11.43 900)
        (effects (font (size 1.27 1.27)))
      )
      (text "CS_GPIO5" (at 1.27 -22.86 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "DC_GPIO16" (at 1.27 -25.4 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "LCD" (at 1.27 -15.24 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "MOSI_GPIO19" (at 1.27 -17.78 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "RST_GPIO23" (at 1.27 -27.94 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "SCLK_GPIO18" (at 1.27 -20.32 0)
        (effects (font (size 1.27 1.27)))
      )
      (text "USB" (at 0 -6.35 0)
        (effects (font (size 1.27 1.27)))
      )
    )
    (symbol "TTGO-T-Display_0_1"
      (rectangle (start -31.75 -2.54) (end 38.1 -60.96)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
    )
    (symbol "TTGO-T-Display_1_1"
      (pin power_in line (at -34.29 -19.05 0) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -46.99 0) (length 2.54)
        (name "GPIO37" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -49.53 0) (length 2.54)
        (name "GPIO36/ADC0" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -34.29 -57.15 0) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -19.05 180) (length 2.54)
        (name "3V3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -21.59 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -24.13 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -31.75 180) (length 2.54)
        (name "GPIO12/ADC15/TOUCH5" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -34.29 180) (length 2.54)
        (name "GPIO13/ADC14/TOUCH4" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -36.83 180) (length 2.54)
        (name "GPIO15/ADC13/TOUCH3" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -39.37 180) (length 2.54)
        (name "GPIO2/ADC12/TOUCH2" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -34.29 -21.59 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -41.91 180) (length 2.54)
        (name "GPIO17" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -44.45 180) (length 2.54)
        (name "GPIO22/I2C_SCL" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.64 -46.99 180) (length 2.54)
        (name "GPIO21/I2C_SDA" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -54.61 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -57.15 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -29.21 0) (length 2.54)
        (name "GPIO27/ADC17/TOUCH7" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -31.75 0) (length 2.54)
        (name "GPIO26/ADC19/DAC2" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -34.29 0) (length 2.54)
        (name "GPIO25/ADC18/DAC1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -36.83 0) (length 2.54)
        (name "GPIO33/ADC5/TOUCH8" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -39.37 0) (length 2.54)
        (name "GPIO32/ADC4/TOUCH9" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -41.91 0) (length 2.54)
        (name "GPIO39/ADC3/SVN" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -34.29 -44.45 0) (length 2.54)
        (name "GPIO38" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
