# SANE-UMAX documentation - supported umax scanner clones
Author: Oliver Rauch
Keywords: umax,scanner,driver,linux,unix,os/2

# SUPPORTED UMAX SCANNER CLONES

#

> The sane-umax library implements a SANE backend that provides acces to several scanners that are compatible to the UMAX-SCSI-protocoll!
> Here is a list of the UMAX-compatible scanners:

UMAX compatible Linotype Hell scanners
Name | Vendor | SCSI-ID | Versions | UTA | ADF | Lineart | Grayscale | Color RGB | Bits/pixel | Optical resolution
Jade | LinoHell | Office | all | X | X | ok | ok | ok | 1,8,24 | 600 x 1200*
Jade2 | LinoHell | Office2 | all | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
Saphir | LinoHell | unknown |  | incl |  |  |  |  | 1,8,10,24,30 | 600 x 1200
Saphir2 | LinoHell | SAPHIR2 | all | incl |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Saphir Ultra | LinoHell | unknown |  | incl |  |  |  |  | 1,8,12,24,36 | 600 x 1200
Saphir Ultra II | LinoHell | unknown |  | incl |  |  |  |  | 1,8,14,24,42 | 1200 x 2400
Saphir HiRes | LinoHell | unknown |  | incl |  |  |  |  | 1,8,14,24,42 | 1220 x 3048 3048 x 3048
Opal | LinoHell | unknown |  | incl |  |  |  |  | 1,8,10,24,30 | 700 x 1400
Opal Ultra | LinoHell | unknown |  | incl |  |  |  |  | 1,8,12,24,36 | 700 x 1400 1400 x 2800

* Scanner is able to scan up to 1200 x 1200 dpi.

UTA = Umax Transparancy Adapter, ADF = Automatic Document Feeder
(X = supported by scanner, incl = is included)

Other UMAX compatible scanners
Name | Vendor | SCSI-ID | Versions | UTA | ADF | Lineart | Grayscale | Color RGB | Bits/pixel | Optical resolution
Vobis/Highscreen Scanboostar Premium | LinoHell | Office2 | all | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
Escom Image Scanner 256 | UMAX | UG80 | all | -- |  | ok | ok | -- | 1,8 | 300 x 300
Nikon AX-210 | Nikon | AX-210 | all(?) | X | X | ok | ok | ok | 1,8,24 | 600 x 1200*
Genius Colorpage HR5 (normal and Pro) | KYE | ColorPage-HR5 | all(?) | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200

* Scanner is able to scan up to 1200 x 1200 dpi.

UTA = Umax Transparancy Adapter, ADF = Automatic Document Feeder
(X = supported by scanner)

SANE-UMAX index

This page has been changed on 1st. july 1999