;
; SANE Backend specification file
;
; It's basically emacs-lisp --- so ";" indicates comment to end of line.
; All syntactic elements are keyword tokens, followed by a string or
;  keyword argument, as specified.
;
; ":backend" *must* be specified.
; All other information is optional (but what good is the file without it?).
;

:backend "plustek"              ; name of backend
:version "0.39"                 ; version of backend
:status :stable                 ; :alpha, :beta, :stable, :new
:manpage "sane-plustek"         ; name of manpage (if it exists)

; backend's web page
:url "http://home.t-online.de/home/g-jaeger/plustek.html"	

:devicetype :scanner            ; start of a list of devices....
                                ; other types:  :stillcam, :vidcam,
                                ;               :meta, :api


:mfg "Plustek"                  ; name of manufacturer
:url "http://www.plustek.com/"

;name models for above-specified mfg.
:model "OpticPro 4800P"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro 4830P"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro 600P/6000P"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro 4831P"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro 9630P"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro 9630PL"
:interface "Parport (SPP, EPP)"
:comment "OK - use driver-switch mov=1"

:model "OpticPro 9600P"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro 1236P"
:interface "Parport (SPP, EPP)"
:comment "OK - reported as OpticPro 12000P/96000P"

:model "OpticPro 12000P/96000P"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro 9636P"
:interface "Parport (SPP, EPP)"
:comment "OK - use driver-switch mov=4"

:model "OpticPro 9636P+/Turbo"
:interface "Parport (SPP, EPP)"
:comment "OK - use driver-switch mov=3"

:model "OpticPro 9636T"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro 12000T"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro AI3"
:interface "Parport (SPP, EPP)"
:comment "OK - use driver-switch mov=5"

:model "OpticPro P8"
:interface "Parport"
:comment "Not tested."

:model "OpticPro P12"
:interface "Parport (SPP, EPP)"
:comment "OK"

:model "OpticPro PT12"
:interface "Parport (SPP, EPP)"
:comment "OK."

:model "OpticPro 19200S"
:interface "SCSI"
:comment "rebadged Artec AM12S (supported by Artec Backend)"

:model "OpticPro 1212U/U12/UT12"
:interface "USB"
:comment "Not supported."

:mfg "Primax"                  ; name of manufacturer
:url "http://www.primax.nl/"

;name models for above-specified mfg.
:model "Colorado 4800"
:interface "Parport (SPP, EPP)"
:comment "Not tested, (same as OP4800P)"

:model "Compact 4800 Direct"
:interface "Parport (SPP, EPP)"
:comment "OK - use driver-switch mov=2"

:model "Compact 4800 Direct-30"
:interface "Parport (SPP, EPP)"
:comment "Not tested, (same as OP4830P)"

:model "Compact 9600 Direct-30"
:interface "Parport (SPP, EPP)"
:comment "OK - (same as OP9630P)"

:mfg "Aries"                  ; name of manufacturer

:model "Scan-It Pro 4800"
:interface "Parport (SPP, EPP)"
:comment "OK - use driver-switch mov=2"

; :comment and :url specifiers are optional after :mfg, :model, :desc,
;  and at the top-level.
