# SANE: Backends (Drivers)

The following table summarizes the backends/drivers distributed with sane-backends-1.0.13, and the hardware or software they support.

This is only a summary! Please consult the manpages and the author-supplied webpages for more detailed (and usually important) information concerning each backend.

If you have new information or corrections, please file a bug report with as many details as possible. Also please tell us if your scanner isn't mentioned in this list at all.

For an explanation of the tables, see the legend.

There are tables for scanners, still cameras, video cameras, APIs, and meta backends.

## Scanners

Backends: abaton, agfafocus, apple, artec, artec_eplus48u, as6e, avision, bh, canon, canon630u, canon_pp, coolscan, coolscan2, epson, fujitsu, gt68xx, hp, hp5400, hpsj5s, ibm, leo, ma1509, matsushita, microtek, microtek2, mustek, mustek_pp, mustek_pp_ccd, mustek_usb, nec, pie, plustek, plustek_pp, ricoh, s9036, sceptre, sharp, sm3600, SnapScan, sp15c, st400, tamarack, teco1, teco2, teco3, umax, umax1220u, umax_pp, unsupported

### Backend: abaton (unmaintained)

Manual page: sane-abaton

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Abaton | Scan 300/GS | SCSI | complete | All known modes and functions supported
Scan 300/S | SCSI | untested | Untested, use with caution

### Backend: agfafocus (unmaintained)

Manual page: sane-agfafocus

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
AGFA | Focus GS Scanner | SCSI | untested | 6 bit gray
Focus Lineart Scanner | SCSI | untested | Lineart only? Untested.
Focus II | SCSI | untested | gray only
Focus Color | SCSI | good | 3-pass
Focus Color Plus | SCSI | good | 3-pass
Siemens | S9036 | SCSI | untested | gray only

### Backend: apple (unmaintained)

Manual page: sane-apple

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Apple | Apple Scanner | SCSI | good | 4bit, 16 shades of gray
OneScanner | SCSI | basic | 8bit, 256 shades of gray. The backend needs work especially in the quantization code but it may work.
ColorOneScanner | SCSI | minimal | truecolor (needs much work) but it scans in non color modes.

### Backend: artec (unmaintained)

Link(s): http://www4.infi.net/~cpinkham/sane/sane-artec-doc.html
Manual page: sane-artec

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Artec/Ultima | AT3 | SCSI | complete | all modes working
A6000C | SCSI | complete | all modes working
A6000C PLUS | SCSI | complete | f/w <= v1.92 basic, f/w >= v1.93 OK
AT6 | SCSI | minimal | First scan works, subsequent fail until scanner power cycle.
AT12 | SCSI | complete | all modes working
AM12S | SCSI | complete | all modes working
BlackWidow | BW4800SP | SCSI | complete | rebadged Artec AT3
Plustek | OpticPro 19200S | SCSI | complete | rebadged Artec AM12S

### Backend: artec_eplus48u (0.0.10)

Link(s): http://www.angelfire.com/linux/crapsite/
Manual page: sane-artec_eplus48u

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Artec/Ultima | E+ 48U | USB | good | CIS scanner based on the GT6816 chip. Apparently all other devices are re-badged Artec scanners.
Medion/Lifetec/Tevion/Cytron | MD9693 | USB | good |
MD9705 | USB | good |
MD4394 | USB | good | Only scanners with product id 0x4003 will work; try the gt68xx backend, if your scanner has product id 0x4002
Trust | Easy Webscan 19200 | USB | good | Different product id: 0x4006
Memorex | MEM 48U | USB | good | Different product id: 0x4005
Microstar | MR 9791 | USB | good |
UMAX | AstraSlim SE | USB | good | Different product id: 0x4009

### Backend: as6e (0.4.2)

Link(s): http://as6edriver.sourceforge.net/
Manual page: sane-as6e

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Artec/Ultima | AS6E | Parport | basic | Requires the program 'as6edriver' to run.

### Backend: avision (Build: 80)

Link(s): http://www.rocklinux-consulting.de/oss/avision/index.html
Manual page: sane-avision

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Avision | AV100CS | SCSI | untested |
AV100IIICS | SCSI | untested |
AV100S | SCSI | untested |
AV210 | USB | untested |
AV220 | USB | untested |
AV240SC | SCSI | untested |
AV260CS | SCSI | untested |
AV360CS | SCSI | untested |
AV363CS | SCSI | untested |
AV420CS | SCSI | untested |
AV6120 | SCSI | untested |
AV610CU Scancopier | USB | untested | 1 pass, 600 dpi
AV620CS | SCSI | complete | 1 pass, 600 dpi
AV620CS Plus | SCSI | complete | 1 pass, 1200 dpi
AV630CS | SCSI | complete | 1 pass, 1200 dpi - regularly tested
AV630CSL | SCSI | untested | 1 pass, 1200 dpi
AV6240 | SCSI | complete | 1 pass, ??? dpi
AV600U | USB | untested | 1 pass, 1200 dpi
AV600U Plus | USB | untested | 1 pass, 1200 dpi
AV660S | USB | untested | 1 pass, 1200 dpi
AV680S | USB | untested | 1 pass, 1200 dpi
AV690U | USB | untested | 1 pass, 2400 dpi
AV800S | SCSI | untested | 1 pass, 1200 dpi
AV810C | SCSI | untested | 1 pass, 1200 dpi
AV820 | SCSI | untested | 1 pass, 1200 dpi
AV820C | SCSI | untested | 1 pass, 1200 dpi
AV820C Plus | SCSI | untested | 1 pass, 1200 dpi
AV830C | SCSI | untested | 1 pass, 1200 dpi
AV830C Plus | SCSI | untested | 1 pass, 1200 dpi
AV880 | SCSI | untested | 1 pass, 1200 dpi
AV880C | SCSI | untested | 1 pass, 1200 dpi
AV8000S | SCSI | complete | 1 pass, 1200 dpi, A3 - regularly tested
AVA3 | SCSI | untested | 1 pass, 600 dpi, A3
Hewlett-Packard | ScanJet 5300C | USB | complete | 1 pass, 1200 dpi - regularly tested
ScanJet 5370C | USB | basic | 1 pass, 2400 dpi
ScanJet 7400c | USB | good | 1 pass, 1200 dpi - dual USB/SCSI interface
ScanJet 7450c | USB | good | 1 pass, 1200 dpi - dual USB/SCSI interface
ScanJet 7490c | USB | good | 1 pass, 1200 dpi - dual USB/SCSI interface
Minolta | FS-V1 | USB | basic | 1 pass, film-scanner
Elite II | USB | untested | 1 pass, film-scanner
Mitsubishi | MCA-ADFC | SCSI | untested |
S1200C | SCSI | untested |
S600C | SCSI | untested |
SS600 | SCSI | good |
Fujitsu | ScanPartner | SCSI | untested |
ScanPartner 10 | SCSI | untested |
ScanPartner 10C | SCSI | untested |
ScanPartner 15C | SCSI | untested |
ScanPartner 300C | SCSI | untested |
ScanPartner 600C | SCSI | untested |
ScanPartner Jr | SCSI | untested |
ScanStation | SCSI | untested |

### Backend: bh (1.0-4)

Link(s): http://www.martoneconsulting.com/sane-bh.html
Manual page: sane-bh
Comment: Supports Copiscan II scanners with Remote SCSI Controller (RSC) interface

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Bell and Howell | COPISCAN II 6338 | SCSI | good | Duplex Scanner with ACE - development model
COPISCAN II 2135 | SCSI | untested | Simplex Scanner
COPISCAN II 2137(A) | SCSI | good | Simplex Scanner (with ACE) - limited testing
COPISCAN II 2138A | SCSI | untested | Simplex Scanner with ACE
COPISCAN II 3238 | SCSI | untested | Simplex Scanner
COPISCAN II 3338(A) | SCSI | untested | Simplex Scanner (with ACE)

### Backend: canon (1.12)

Link(s): http://www.rzg.mpg.de/~mpd/sane/
Manual page: sane-canon

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Canon | CanoScan 300 | SCSI | good | 1 pass; flatbed scanner
CanoScan 600 | SCSI | good |
CanoScan 620S | SCSI | good | 1 pass; flatbed scanner
CanoScan 1200S | SCSI | good | 1 pass; flatbed scanner
CanoScan 2700F | SCSI | good | 1 pass; film scanner
CanoScan 2710S | SCSI | good | 1 pass; 36bit film scanner

### Backend: canon630u (0.1)

Link(s): http://canon-fb630u.sourceforge.net/
Manual page: sane-canon630u

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Canon | CanoScan fb630u | USB | good | OK
CanoScan fb636u | USB | untested | hopefully works

### Backend: canon_pp (0.32)

Link(s): http://canon-fb330p.sourceforge.net
Manual page: sane-canon_pp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Canon | CanoScan FB310P | Parport (ECP) | unsupported | Rebadged Avision, different command set
CanoScan FB610P | Parport (ECP) | unsupported | Rebadged Avision, different command set
CanoScan FB320P | Parport (ECP) | basic | Newly added support
CanoScan FB620P | Parport (ECP) | basic | Newly added support
CanoScan FB330P | Parport (ECP) | good |
CanoScan FB630P | Parport (ECP) | good |
CanoScan N340P | Parport (ECP) | good |
CanoScan N640P | Parport (ECP) | good |
CanoScan N640P ex | Parport (ECP) | good | Just an N640P in a different box?

### Backend: coolscan (0.4.3)

Link(s): http://andreas.rick.free.fr/sane/
Manual page: sane-coolscan

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Nikon | LS-20 | SCSI | basic | The LS-20 has been replaced by the LS-30
LS-30 | SCSI | basic | alpha: only 24/30 bit RGB + 32/40 bit RGBI
LS-2000 | SCSI | basic | alpha: only 24/36 bit + RGB 32/48 bit RGBI
LS-1000 | SCSI | basic | Doesn't support gamma correction

### Backend: coolscan2 (0.1.8)

Link(s): http://coolscan2.sourceforge.net/
Manual page: sane-coolscan2

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Nikon | LS 30 | SCSI | complete | working -- model available to developer
LS 2000 | SCSI | good |
LS 40 ED | USB | complete |
LS 4000 ED | IEEE-1394 | good | needs linux kernel 2.4.19 or later
LS 8000 ED | IEEE-1394 | good | needs linux kernel 2.4.19 or later

### Backend: epson (0.2.32)

Link(s): http://www.khk.net/sane
Manual page: sane-epson

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Epson | GT-5000 | Parport | good |
Actionscanner II | Parport | good | US version of GT-5000
GT-6000 | SCSI Parport | good |
ES-300C | SCSI Parport | good | US version of GT-6000
GT-5500 | SCSI | good |
GT-6500 | Parport | good |
ES-600C | Parport | good | US version of GT-6500
ES-1200C | Parport | good | US version of GT-9000
GT-7000 | SCSI | good |
GT-8000 | SCSI | good |
ES-8500 | SCSI | good |
Perfection 636S | SCSI | complete | US version of GT-7000
Perfection 636U | USB | complete |
Perfection 610 | USB | complete |
Perfection 640 | USB | complete |
Perfection 1200S | SCSI | complete |
Perfection 1200U | USB | complete |
Perfection 1200Photo | USB | complete | with TPU
Perfection 1240 | SCSI USB | complete |
Perfection 1640 | SCSI USB | complete |
Perfection 1650 | USB | complete |
Perfection 1660 | USB | complete |
Perfection 2400 | USB | complete |
Perfection 2450 | USB IEEE-1394 | complete |
Perfection 3200 | USB | complete | US version of the GT-9800
Expression 636 | SCSI | complete | US version of GT-9500
Expression 800 | SCSI | complete |
Expression 1600 | SCSI USB IEEE-1394 | complete |
Expression 1680 | SCSI USB IEEE-1394 | complete |
FilmScan 200 | SCSI | unsupported | A better backend for the FilmScan 200 can be found at http://www.vjet.demon.co.uk/scanner/
CX-3200 | USB | untested |
CX-5200 | USB | untested |

### Backend: fujitsu (1.12)

Manual page: sane-fujitsu

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Fujitsu | M3096G | SCSI | good |
M3091DCd | SCSI | good |
M3092DCd | SCSI | good |
M3093GXim | SCSI | good |
M3093GDim | SCSI | good |
M4097 | SCSI | good |
fi-4110EOX2 | USB | unsupported |
fi-4120C | SCSI USB | good |
fi-4220C | SCSI USB | good |
fi-4340C | SCSI USB | good |
ScanPartner 93GX | SCSI | good |
fi-4530C | SCSI | basic | color scan returns inverted image, Flatbed option is enabled

### Backend: gt68xx (1.0-49)

Link(s): http://www.meier-geinitz.de/sane/gt68xx-backend/
Manual page: sane-gt68xx
Comment: Only the USB scanners mentioned below are supported. For other Mustek BearPaws, look at the Plustek and the MA-1509 backend.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Artec/Ultima | Ultima 2000 | USB | good | Works, only product id 0x4002 is supported
Ultima 2000 e+ | USB | good | Works, only limited testing until now
Boeder | Sm@rtScan Slim Edition | USB | good | Similar to Artec Ultima 2000
Fujitsu | 1200CUS | USB | basic | Works, but is slow. Maybe a Mustek BearPaw 2400 CU clone?
Genius | Colorpage Vivid3x | USB | good | Works but has limited testing
Colorpage Vivid3xe | USB | basic | Works but has limited testing. Color problems? Reports are welcome.
Colorpage Vivid4x | USB | untested | Should be detecetd but may not work. Please contact me if you have such a scanner.
Lexmark | X70 | USB | good | Works, some resolutions fail at 16 bit
X73 | USB | good | Works, some resolutions fail at 16 bit, same as X70
Medion/Lifetec/Tevion/Cytron | MD 4394 | USB | good | Product id 0x4002. If you have 0x4003, use artec_eplus48u backend.
MD/LT 9375 | USB | untested | Untested, but is reported to have the same ids as the Artec Ultima 2000. Please test.
MD/LT 9385 | USB | good | Similar to Artec Ultima 2000
LT 9452 | USB | good | Similar to Mustek ScanExpress 1200 UB Plus
MD 9458 | USB | good | Similar to Artec Ultima 2000 (e+?)
Mustek | BearPaw 1200 CS | USB | good |
BearPaw 1200 CU | USB | good |
BearPaw 1200 CU Plus | USB | good |
BearPaw 1200 TA | USB | good | Transparency adapter supported
BearPaw 2400 CS | USB | untested | Probably works, reports are welcome
BearPaw 2400 CS Plus | USB | good | Works, problems with 12/16 bit modes?
BearPaw 2400 CU | USB | basic | Works, but is slow
BearPaw 2400 CU Plus | USB | good |
BearPaw 2400 TA | USB | good | Transparency adapter supported
BearPaw 2400 TA Plus | USB | good | Transparency adapter supported
ScanExpress 1200 UB Plus | USB | good |
ScanExpress A3 USB | USB | good | Should work. I've only few reports so please contact me, if you own such a device and tell me, if you find any problems
ScanExpress 2400 USB | USB | minimal | Should be detected but may need some more work in the code. Testers welcome.
ScanMagic 1200 UB Plus | USB | good | Same as ScanExpress 1200 UB Plus
Packard Bell | Diamond 1200 | USB | good | Similar to Mustek BearPaw 1200 (Plus)
Diamond 1200 Plus | USB | good | Similar to Mustek BearPaw 1200 Plus
Plustek | OpticPro 1248U | USB | good | Works up to 600 dpi.
OpticSlim 1200 | USB | good |
OpticPro U16B | USB | untested | Should be detected but may not work. Please contact me if you own such a device.
OpticPro UT16B | USB | untested | Should be detected but may not work. Please contact me if you own such a device. Same as U16B but with a transparency adapter?
RevScan | 19200i | USB | good | Similar to Plustek OpticPro 1248U
Trust | Flat Scan USB 19200 | USB | good | Similar to Artec Ultima 2000
Compact Scan USB 19200 | USB | good | Works, if you have vendor id 0x055f and product id 0x0006, use the mustek_usb backend instead, similar to Mustek ScanExpress 1200 UB (Plus)

### Backend: hp (1.05)

Link(s): http://www.kirchgessner.net/
Manual page: sane-hp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Hewlett-Packard | ScanJet Plus | Propietary | complete | Driver for HP parallel interface card required
ScanJet IIc | SCSI | complete |
ScanJet IIp | SCSI | complete |
ScanJet IIcx | SCSI | complete |
ScanJet 3c | SCSI | complete |
ScanJet 3p | SCSI | complete |
ScanJet 4c | SCSI | complete |
ScanJet 4p | SCSI | complete |
ScanJet 4100C | USB | complete |
ScanJet 5p | SCSI | complete |
ScanJet 5100C | Parport | complete | Requires ppscsi driver and epst module
ScanJet 5200C | Parport USB | complete | Parallel interface requires ppscsi driver and epst module
ScanJet 6100C | SCSI | complete |
ScanJet 6200C | SCSI USB | complete |
ScanJet 6250C | SCSI USB | complete |
ScanJet 6300C | SCSI USB | complete |
ScanJet 6350C | SCSI USB | complete |
ScanJet 6390C | SCSI USB | complete |
PhotoSmart PhotoScanner | SCSI | complete |

### Backend: hp5400 (1.0-2)

Link(s): http://sourceforge.net/projects/hp5400backend
Manual page: sane-hp5400
Comment: HP5400 and HP5470 scanners. Prototype backend available

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 5400c | USB | basic |
ScanJet 5470c | USB | basic |
ScanJet 5490c | USB | basic |

### Backend: hpsj5s (0.03)

Link(s): http://hpsj5s.sourceforge.net/
Manual page: sane-hpsj5s

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Hewlett-Packard | ScanJet 5s | Parport (EPP) | minimal | Requires libieee1284 library. Only gray mode.

### Backend: ibm (1.0-4)

Link(s): http://www.meier-geinitz.de/sane/ibm-backend/
Manual page: sane-ibm
Comment: This backend has had only limited testing. It needs more work especially for the Ricoh scanners. Patches are welcome.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
IBM | 2456 | SCSI | basic | Was reported to work long time ago. Reports are welcome.
Ricoh | IS-410 | SCSI | untested | Untested, please report!
IS-420 | SCSI | basic | Works at least in flatbed mode.
IS-430 | SCSI | untested | Untested, please report!

### Backend: leo (1.0-10)

Link(s): http://www.zago.net/sane/#leo
Manual page: sane-leo

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
LEO | LEOScan S3 | SCSI | good | FCC ID LUZFS1130
Across Technologies | FS-1130 | SCSI | good | FCC ID LUZFS1130
Genius | FS-1130 Colorpage Scanner | SCSI | untested |

### Backend: ma1509 (1.0-3)

Link(s): http://www.meier-geinitz.de/sane/ma1509-backend/
Manual page: sane-ma1509

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Mustek | BearPaw 1200 F | USB | good | Works upto 600 dpi. No support for TA and ADF yet.

### Backend: matsushita (1.0-6)

Link(s): http://www.zago.net/sane
Manual page: sane-matsushita

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Panasonic | KV-SS25 | SCSI | complete |
KV-SS25D | SCSI | complete |
KV-SS50 | SCSI | untested |
KV-SS55 | SCSI | untested |
KV-SS50EX | SCSI | untested |
KV-SS55EX | SCSI | untested |
KV-SS850 | SCSI | untested |
KV-SS855 | SCSI | untested |

### Backend: microtek (0.13.1)

Link(s): http://www.mir.com/mtek/
Manual page: sane-microtek

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Microtek | Scanmaker E6 | SCSI | good |
Scanmaker E3 | SCSI | good |
Scanmaker E2 | SCSI | good | 3-pass
Scanmaker 35t+ | SCSI | good | slide-scanner
Scanmaker 45t | SCSI | good | slide-scanner
Scanmaker 35 | SCSI | good | slide-scanner
Scanmaker III | SCSI | good |
Scanmaker IISP | SCSI | good |
Scanmaker IIHR | SCSI | good | 3-pass
Scanmaker IIG | SCSI | good | gray only
Scanmaker II | SCSI | good | 3-pass
Scanmaker 600Z(S) | SCSI | untested |
Scanmaker 600G(S) | SCSI | basic | gray only (see manpage)
Color PageWiz | SCSI (Parport) | basic | sheet-fed (preliminary, see mapage)
Agfa | Arcus II | SCSI | good | Arcus *II*, not Arcus!
StudioScan | SCSI | good |
StudioScan II | SCSI | good |
StudioScan IIsi | SCSI | good |
DuoScan | SCSI | basic |
Vobis | Highscreen Realscan | SCSI | good |
Genius | Colorpage-SP2 | SCSI | good | Same as Microtek Scanmaker E3

### Backend: microtek2 (0.95)

Link(s): http://karstenfestag.gmxhome.de
Manual page: sane-microtek2

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Microtek | ScanMaker E3plus | Parport | complete |
ScanMaker E3plus | SCSI | complete |
ScanMaker X6 | SCSI | complete |
ScanMaker X6EL | SCSI | basic |
ScanMaker X6USB | USB | good |
ScanMaker V300 | SCSI | good |
ScanMaker V300 | Parport | good |
ScanMaker V310 | SCSI | basic |
ScanMaker V310 | Parport | basic |
ScanMaker V600 | SCSI | basic |
ScanMaker V600 | Parport | basic |
ScanMaker 330 | SCSI | basic |
ScanMaker 630 | SCSI | basic |
ScanMaker 636 | SCSI | complete |
ScanMaker 9600XL | SCSI | good | only flatbed mode ?
Phantom 330CX | Parport | complete |
SlimScan C3 | Parport | complete |
Phantom 636 | SCSI | complete |
Phantom 636CX | Parport | complete |
SlimScan C6 | USB | complete |
ScanMaker V6USL | SCSI | complete |
ScanMaker V6USL | USB | complete |
ScanMaker X12USL | SCSI | good | only Flatbed mode ?
Vobis | HighScan | SCSI | complete | only E3plus based models
Scanport | SQ300 | Parport? | basic |
SQ2030 | Parport | basic |
SQ4836 | SCSI | basic |

### Backend: mustek (1.0-134)

Link(s): http://www.meier-geinitz.de/sane/mustek-backend/
Manual page: sane-mustek
Comment: Most Mustek SCSI scanners are supported by this backend. For USB scanners, look at the mustek_usb backend.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Mustek | Paragon MFS-6000CX | SCSI | good | 3-pass
Paragon MFS-12000CX | SCSI | good | 3-pass
Paragon MFC-600S | SCSI | complete |
Paragon 600 II CD | SCSI | complete |
ScanMagic 600 II SP | SCSI | complete |
Paragon MFC-800S | SCSI | complete |
Paragon 800 II SP | SCSI | complete |
Paragon MFS-6000SP | SCSI | complete |
Paragon MFS-8000SP | SCSI | complete |
Paragon MFS-1200SP | SCSI | complete |
Paragon MFS-12000SP | SCSI | complete |
ScanExpress 6000SP | SCSI | complete |
ScanExpress 12000SP | SCSI | complete |
ScanExpress 12000SP Plus | SCSI | complete |
Paragon 1200 III SP | SCSI | complete |
Paragon 1200 LS | SCSI | complete |
ScanMagic 9636S | SCSI | complete |
ScanMagic 9636S Plus | SCSI | complete |
ScanExpress A3 SP | SCSI | basic | Please test!
Paragon 1200 SP Pro | SCSI | good |
Paragon 1200 A3 Pro | SCSI | good |
Paragon 600 II N | Proprietary | basic | Resolutions above 300 dpi may cause trouble.
Trust | Imagery 1200 | SCSI | good | 3-pass, Mustek Paragon MFS-6000CX compatible
Imagery 1200 SP | SCSI | complete | Mustek Paragon MFS-6000SP compatible
Imagery 4800 SP | SCSI | complete | Mustek Paragon 600 II CD compatible
SCSI Connect 19200 | SCSI | complete | Mustek ScanExpress 12000SP compatible
SCSI excellence series 19200 | SCSI | complete | Mustek ScanExpress 12000SP compatible
Primax | Compact 4800 SCSI | SCSI | complete | Mustek 600 II CD compatible

### Backend: mustek_pp (12)

Link(s): http://penguin-breeder.org/?page=mustek_pp
Manual page: sane-mustek_pp
Comment: Supports CIS type parallel port scanners from Mustek. A lot of Mustek CCD scanners are supported by the mustek_pp_ccd backend.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Mustek | 96 CP | Parport (EPP) | good | 300x600 dpi CIS scanner
ScanExpress 600 CP | Parport (EPP) | good | 300x600 dpi CIS scanner
ScanMagic 600 CP | Parport (EPP) | good | 300x600 dpi CIS scanner
ScanExpress 1200 CP | Parport (EPP) | good | 600x1200 dpi CIS scanner
ScanExpress 1200 CP+ | Parport (EPP) | good | 600x1200 dpi CIS scanner
Medion/Lifetec/Tevion/Cytron | MD/LT 935x | Parport (EPP) | good | 600x1200 dpi CIS scanner
MD/LT 985x | Parport (EPP) | good | 600x1200 dpi CIS scanner
MD/LT 9890 | Parport (EPP) | good | 600x1200 dpi CIS scanner
Targa | Funline TS12 EP | Parport (EPP) | good | 600x1200 dpi CIS scanner
Funline TS6 EP | Parport (EPP) | good | 300x600 dpi CIS scanner
Trust | Easy Connect 9600+ | Parport (EPP) | good | 300x600 dpi CIS scanner
Easy Connect 19200+ | Parport (EPP) | good | 300x600 dpi CIS scanner

### Backend: mustek_pp_ccd (9)

Link(s): http://www.penguin-breeder.org/?page=mustek_pp
Manual page: sane-mustek_pp_ccd
Comment: Supports CCD type parallel port scanners from Mustek. A lot of Mustek CIS scanners are supported by the mustek_pp backend.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Mustek | ScanExpress 6000 P | Parport (EPP) | good | works
ScanMagic 4800 P | Parport (EPP) | good | works
ScanExpress 1200 ED Plus | Parport (EPP) | minimal | works partly
ScanMagic 1200 ED Plus | Parport (EPP) | minimal | works partly
600 III EP Plus | Parport (SPP,EPP) | good | works
ScanExpress 600 SEP | Parport (EPP) | good | works
Medion/Lifetec/Tevion/Cytron | MD9848 | Parport (SPP) | good | aka. ``Aldi Scanner'' - works
Fidelity Imaging Solutions Inc. | Gallery 4800 | Parport (EPP) | good | works

### Backend: mustek_usb (1.0-17)

Link(s): http://www.meier-geinitz.de/sane/mustek_usb-backend/
Manual page: sane-mustek_usb
Comment: Only the USB scanners mentioned below are supported. For BearPaws, look at the Plustek, MA-1509, and gt68xx backends.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Mustek | ScanExpress 600 CU | USB | complete |
ScanExpress 1200 CU | USB | complete |
ScanExpress 1200 CU Plus | USB | complete |
ScanExpress 1200 UB | USB | complete | For the UB Plus, see gt68xx backend
Trust | Compact Scan USB 19200 | USB | complete | Mustek 1200 UB compatible

### Backend: nec (0.12)

Link(s): http://www5a.biglobe.ne.jp/~saetaka/
Manual page: sane-nec

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
NEC | PC-IN500/4C | SCSI | good | PC-IN500/4C was sold only in JAPAN

### Backend: pie (1.0)

Link(s): http://www.munton.demon.co.uk/sane
Manual page: sane-pie

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Devcom | 9636PRO | SCSI | good |
9636S | SCSI | untested |
9630S | SCSI | untested |
PIE | ScanAce 1236S | SCSI | good |
ScanAce 1230S | SCSI | good |
ScanAce II | SCSI | untested |
ScanAce III | SCSI | good |
ScanAce Plus | SCSI | untested |
ScanAce II Plus | SCSI | untested |
ScanAce III Plus | SCSI | untested |
ScanAce V | SCSI | untested |
ScanAce ScanMedia | SCSI | untested |
ScanAce ScanMedia II | SCSI | untested |
ScanAce 630S | SCSI | untested |
ScanAce 636S | SCSI | untested |
Adlib | JetScan630 | SCSI | good |
JetScan636PRO | SCSI | untested |

### Backend: plustek (0.46)

Link(s): http://www.gjaeger.de/scanner/plustek.html
Manual page: sane-plustek

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Plustek | OpticPro U12 | USB | complete | NOTE: Devices with product ID 0x0001 are not supported!
OpticPro UT12 | USB | complete | Note: Devices with product ID 0x0001 are not supported!
OpticPro UT16 | USB | complete |
OpticPro U24 | USB | complete |
OpticPro UT24 | USB | complete |
OpticPro 19200S | SCSI | unsupported | rebadged Artec AM12S (supported by Artec Backend)
Genius | Colorpage HR6 V2 | USB | complete |
Colorpage HR7 | USB | complete |
Colorpage HR6A | USB | untested |
Colorpage HR7LE | USB | untested |
Colorpage HR6X | USB | untested |
Mustek | BearPaw 1200 | USB | complete |
BearPaw 2400 | USB | complete |
Hewlett-Packard | ScanJet 2100C | USB | complete |
ScanJet 2200C | USB | complete |
Epson | Perfection 1250 | USB | complete |
Perfection 1250Photo | USB | good | TPA scans not perfect
Perfection 1260 | USB | complete |
Perfection 1260Photo | USB | good | TPA scans not perfect
Umax | UMAX 3400 | USB | complete |
UMAX 3450 | USB | good | TPA not supported
UMAX 5400 | USB | complete |
Compaq | S4-100 | USB | complete | Identical to UMAX 3400
Canon | CanoScan N650U/N656U | USB | complete |
CanoScan N1220U | USB | complete |
CanoScan N670U/N676U | USB | complete |
CanoScan N1240U | USB | complete |
CanoScan LiDE20 | USB | complete |
CanoScan LiDE30 | USB | complete |

### Backend: plustek_pp (0.01)

Link(s): http://www.gjaeger.de/scanner/plustek.html
Manual page: sane-plustek_pp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Plustek | OpticPro 4800P | Parport (SPP, EPP) | complete |
OpticPro 4830P | Parport (SPP, EPP) | complete |
OpticPro 600P/6000P | Parport (SPP, EPP) | complete |
OpticPro 4831P | Parport (SPP, EPP) | complete |
OpticPro 9630P | Parport (SPP, EPP) | complete |
OpticPro 9630PL | Parport (SPP, EPP) | complete | use driver-switch mov=1
OpticPro 9600P | Parport (SPP, EPP) | complete |
OpticPro 1236P | Parport (SPP, EPP) | complete | reported as OpticPro 12000P/96000P
OpticPro 12000P/96000P | Parport (SPP, EPP) | complete |
OpticPro 9636P | Parport (SPP, EPP) | complete | use driver-switch mov=4
OpticPro 9636P+/Turbo | Parport (SPP, EPP) | complete | use driver-switch mov=3
OpticPro 9636T | Parport (SPP, EPP) | complete |
OpticPro 12000T | Parport (SPP, EPP) | complete |
OpticPro AI3 | Parport (SPP, EPP) | basic | use driver-switch mov=5, poor picture quality
OpticPro P8 | Parport | untested |
OpticPro P12 | Parport (SPP, EPP) | complete |
OpticPro PT12 | Parport (SPP, EPP) | complete |
Primax | Colorado 4800 | Parport (SPP, EPP) | untested | same as OpticPro 4800P
Compact 4800 Direct | Parport (SPP, EPP) | complete | use driver-switch mov=2
Compact 4800 Direct-30 | Parport (SPP, EPP) | complete | same as OpticPro 4830P, use driver-switch mov=7
Compact 9600 Direct-30 | Parport (SPP, EPP) | complete | same as OpticPro 9630P
Genius | Colorpage Vivid III V2 | Parport (SPP, EPP) | complete | Reported as PT12
Colorpage Vivid Pro II Film | Parport (SPP, EPP) | complete | Reported as OP9636T/12000T
Colorpage HR6X EPP | Parport (SPP, EPP) | untested |
Aries | Scan-It Pro 4800 | Parport (SPP, EPP) | complete | use driver-switch mov=2
BrightScan | BrighScan OpticPro | Parport (SPP, EPP) | complete | Reported as P12

### Backend: ricoh (unmaintained)

Manual page: sane-ricoh

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Ricoh | Ricoh IS50 | SCSI | basic |
Ricoh IS60 | SCSI | basic |

### Backend: s9036 (unmaintained)

Manual page: sane-s9036

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Siemens | 9036 Flatbed scanner | SCSI | basic |

### Backend: sceptre (1.0-10)

Link(s): http://www.zago.net/sane/
Manual page: sane-sceptre

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Sceptre | Vividscan S1200 | SCSI | basic |
Komodo | S1200 | SCSI | untested | rebadged Sceptre S1200

### Backend: sharp (0.32)

Link(s): http://www.satzbau-gmbh.de/staff/abel/sane-sharp.html
Manual page: sane-sharp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Sharp | JX-610 | SCSI | good |
JX-250 | SCSI | good |
JX-320 | SCSI | good |
JX-325 | SCSI | untested |
JX-330 | SCSI | good |
JX-350 | SCSI | good |

### Backend: sm3600 (0.1)

Link(s): http://sm3600.sourceforge.net/
Manual page: sane-sm3600

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Microtek | ScanMaker 3600 | USB | basic | works
ScanMaker 3700 | USB | basic | works
ScanMaker 3750 | USB | basic | works (told)

### Backend: SnapScan (1.4)

Link(s): http://snapscan.sourceforge.net/
Manual page: sane-snapscan
Comment: Supported bit depths: 24 bit (color), 8 bit (gray)

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
AGFA | SnapScan | SCSI | good |
SnapScan 300 | SCSI | good |
SnapScan 310 | SCSI | good |
SnapScan 600 | SCSI | good | Optional ADF supported.
Arcus 1200 | SCSI | good | Optional transparency unit supported.
SnapScan 1236s | SCSI | good | Optional ADF and transparency unit supported.
SnapScan 1236u | USB | good | Optional ADF and transparency unit supported.
SnapScan 1212u | USB | good |
SnapScan e10 | USB | good |
SnapScan e20 | USB | good |
SnapScan e25 | USB | good |
SnapScan e26 | USB | good |
SnapScan e40 | USB | good |
SnapScan e42 | USB | good |
SnapScan e50 | USB | good | Optional tranparency unit supported
SnapScan e52 | USB | good | Optional tranparency unit supported
SnapScan e60 | USB | untested |
Benq | 300f | SCSI | good |
310s | SCSI | good |
610s | SCSI | good |
610plus | SCSI | good |
620s | SCSI | good |
310u | USB | good |
320u | USB | good |
340u | USB | good |
620u | USB | good | Optional tranparency unit supported
640u | USB | good | Optional tranparency unit supported
640bu | USB | good |
1240 | USB | good | Optional tranparency unit supported
3300 | USB | good |
4300 | USB | good |
5000 | USB | basic | Working up to 600 DPI
5300 | USB | basic | Problems with firmware upload reported
Guillemot / Hercules | Maxi Scan A4 Deluxe (SCSI) | SCSI | good | Rebadged SnapScan 310s.
Scan@home Touch 1248 (USB) | USB | good | Rebadged Benq 3300.
Maxi Scan A4 USB 640U | USB | good | Rebadged Benq 640U.
Mitsubishi | Diamondview 648UT | USB | good | Rebadged Benq 320u.
Diamondview 650U | USB | good | Rebadged Benq 4300.
Epson | Perfection 660 | USB | good |
Perfection 1670 | USB | basic |

### Backend: sp15c (unmaintained)

Manual page: sane-sp15c

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Fujitsu | SP15C | SCSI | good |

### Backend: st400 (1.6)

Link(s): http://www.informatik.uni-oldenburg.de/~ingo/sane/
Manual page: sane-st400

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Siemens | ST400 | SCSI | basic | 6 bit gray
ST800 | SCSI | basic | 6 bit gray

### Backend: tamarack (unmaintained)

Manual page: sane-tamarack

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Tamarack | Artiscan 6000C | SCSI | good | 3 pass, 300 DPI
Artiscan 8000C | SCSI | good | 3 pass, 400 DPI
Artiscan 12000C | SCSI | good | 3 pass, 600 DPI

### Backend: teco1 (1.0-9)

Link(s): http://www.zago.net/sane/#teco
Manual page: sane-teco1

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Relisys | RELI 2412 | SCSI | complete | sub model VM3530+
AVEC 2400 | SCSI | complete | sub model VM3520
RELI 4830 | SCSI | good | sub model VM4542
AVEC 2412 | SCSI | untested | sub model VM3520+
AVEC 4800 | SCSI | untested | sub model VM4530
AVEC 4816 | SCSI | untested | sub model VM4530+
RELI DS6 | SCSI | untested | sub model VM3420
RELI DS15 | SCSI | untested | sub model VM3440
RELI 2400 | SCSI | untested | sub model VM3530
RELI 4816 | SCSI | untested | sub model VM4540
RELI 9600 | SCSI | untested | sub model VM6530
RELI 9612 | SCSI | untested | sub model VM6530*
RELI 9624 | SCSI | untested | sub model VM6530+
RELI 9630 | SCSI | untested | sub model VM6540
Actown | ACT Scan I 30 | SCSI | untested | sub model VM3520A
Dextra | DF-600P | SCSI | good | sub model VM3510
DF-1200T+ | SCSI | untested | sub model VM3530+
DF-4830T | SCSI | untested | sub model VM4542
DF-9624 | SCSI | untested | sub model VM6530+

### Backend: teco2 (1.0-6)

Link(s): http://www.zago.net/sane/#teco2
Manual page: sane-teco2

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Relisys | AVEC Super 3 | SCSI | untested | sub model VM3575
AVEC II S3 | SCSI | basic | sub model VM3564
SCORPIO Super 3 | SCSI | basic | sub model VM3575
APOLLO Express 3 | SCSI | basic | sub model VM356A
APOLLO Express 6 | SCSI | good | sub model VM6565
SCORPIO Pro | SCSI | good | sub model VM6575
SCORPIO Pro-S | SCSI | untested | sub model VM6586
Primax | Jewel 4800 | SCSI | basic | sub model VM356A
Profi 9600 | SCSI | basic | sub model VM6575
Profi 19200 | SCSI | good | sub model VM6586
Mustek | ScanMagic 4830S | SCSI | untested | sub model VM3575

### Backend: teco3 (1.0-1)

Link(s): http://www.zago.net/sane/#teco3
Manual page: sane-teco3

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Relisys | Infinity Scorpio | SCSI | good | sub model VM3552
Plustek | OpticPro 2400SP | SCSI | untested | sub model VM3552
PIOTECH | Splendeur 3024 | SCSI | good | sub model VM3552
Trust | Imagery 2400 SP | SCSI | good | sub model VM3552
Imagery 4800 SP+ | SCSI | good | sub model VM3552
Imagery 9600 SP | SCSI | untested | sub model VM3552

### Backend: umax (1.0-40)

Link(s): http://www.rauch-domain.de/sane-umax/index.html
Manual page: sane-umax

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
UMAX | Vista S6 | SCSI | good | OK
Vista S6E | SCSI | good | OK
UMAX S-6E | SCSI | good | OK
UMAX S-6EG | SCSI | good | OK
Vista-S8 | SCSI | good | OK
Supervista S-12 | SCSI | good | OK
UMAX S-12 | SCSI | good | OK
UMAX S-12G | SCSI | good | OK
Astra 600S | SCSI | good | OK
Astra 610S | SCSI | good | OK
Astra 1200S | SCSI | good | OK
Astra 1220S | SCSI | good | OK
Astra 2100S | SCSI | good | OK
Astra 2200 (SU) | SCSI | good | OK
Astra 2200 (SU) | USB | good | OK, needs USB control messages
Astra 2400S | SCSI | good | OK
Astra 6400 | IEEE-1394 | unsupported | will propably work one day
Astra 6450 | IEEE-1394 | unsupported | will propably work one day
Astra MX3 | SCSI | good | OK
Astra MX3 | USB | good | OK, needs USB control messages
Mirage D-16L | SCSI | good | OK
Mirage II | SCSI | good | OK
Mirage IIse | SCSI | good | OK
PSD | SCSI | good | OK
PowerLook | SCSI | good | OK, SCSI-ID=PS-2400X
PL-II | SCSI | good | OK
PowerLook III | SCSI | good | OK
PowerLook 270 | SCSI | unsupported | incompatible
PowerLook 270plus | SCSI | unsupported | incompatible
PowerLook 1100 | IEEE-1394 | unsupported | will propably work one day
PowerLook 2000 | SCSI | good | OK
PowerLook 2100XL | SCSI | good | OK
PowerLook 3000 | SCSI | good | OK
Gemini D-16 | SCSI | good | OK
UMAX VT600 | SCSI | untested | may work, please test and give feedback
Vista-T630 | SCSI | good | OK for some firmwareversions, on others only lineart OK
UC 630 | SCSI | good | Version 2.8 OK, others only lineart OK
UG 630 | SCSI | good | OK
UG 80 | SCSI | good | OK
UC 840 | SCSI | good | Version 1.6 OK, others only lineart OK
UC 1200S | SCSI | untested | may work, please test and give feedback
UC 1200SE | SCSI | good | Version 3.0 OK, others unknown
UC 1260 | SCSI | good | Version 1.6 OK, others unknown
Linotype Hell | Jade | SCSI | good | OK, SCSI-ID=LinoHell Office
Jade | SCSI | good | OK, SCSI-ID=LinoHell JADE
Jade2 | SCSI | good | OK, SCSI-ID=LinoHell Office2
Saphir | SCSI | untested | support disabled until tested - please contact author
Saphir2 | SCSI | good | OK, SCSI-ID=LinoHell SAPHIR2
Saphir3 | SCSI | good | OK, SCSI-ID=LinoHell SAPHIR3
Saphir Ultra | SCSI | untested | support disabled until tested - please contact author
Saphir Ultra II | SCSI | good | OK, SCSI-ID=Linotype SAPHIR4
Saphir HiRes | SCSI | untested | support disabled until tested - please contact author
Opal | SCSI | untested | support disabled until tested - please contact author
Opal Ultra | SCSI | untested | support disabled until tested - please contact author
Linoscan 1400 | SCSI | good | OK, SCSI-ID=HDM LS4H1S
Vobis | Highscreen Scanboostar Premium | SCSI | good | OK, SCSI-ID=LinoHell Office2
EDGE | KTX-9600US | SCSI | untested | no feedback
Epson | Perfection 600 | SCSI | good | OK, SCSI-ID=EPSON Perfection600
Escom | Image Scanner 256 | SCSI | good | OK, SCSI-ID=UMAX UG 80
Escort | Galleria 600 | SCSI | untested | untested, SCSI-ID=ESCORT Galleria 600S
Genius | ColorPage-HR5 (Pro) | SCSI | good | OK, SCSI-ID=KYE ColorPage-HR5
Nikon | AX-110 / Scantouch 110 | SCSI | untested | may work, please test and give feedback
AX-210 | SCSI | good | OK
TriGem | PowerScanII | SCSI | good | OK

### Backend: umax1220u (1.0.1)

Link(s): http://umax1220u-sane.sourceforge.net
Manual page: sane-umax1220u

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
UMAX | Astra 1220U | USB | good | OK
Astra 2000U | USB | minimal | Sort of scans, but colors all messed up.

### Backend: umax_pp (1)

Link(s): http://umax1220p.sourceforge.net/
Manual page: sane-umax_pp

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
UMAX | Astra 1220P | Parport (EPP) | good |
Astra 2000P | Parport (EPP) | good |
Astra 1600P | Parport (EPP) | good |
Astra 610P | Parport (EPP) | unsupported | don't work due to lack of hardware to test
Hewlett-Packard | Scanjet 3200C | Parport (EPP) | good | works (relabelled 1220P and 2000P)

### Backend: unsupported (2003-11-15)

Link(s): /contrib.html
Comment: The devices mentioned here are not supported by any SANE backend. However, there may be links to information about them or stand-alone programs.

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Artec/Ultima | 1236 USB | USB | unsupported | Unsupported. Vendor/product 0x05d8/0x4001. See link for details.
AM12e+ | Parport | unsupported | Unsupported. Chipset unknown. Maybe similar to SCSI version or as6e?
E+ Pro | USB | unsupported | Not supported. Vendor/product 0x05d8/0x4004. /proc/bus/usb/devices output is available. Chipset is GT6816. May work with the gt68xx backend after some work in the source code.
Ultima 2000 (0x4001) | USB | unsupported | Same name, but different ids: vendor/product 0x05d8/0x4001 is not supported. The scanner with product id 0x4002 is supported by the gt68xx backend.
Avision | iVina FB1600 | USB | unsupported | Not supported. GL646. Same as UMAX Astra 4500. A backend is currenly beeing developed.
iVina FB1800 | USB | unsupported | Not supported. GL660 + GL646. Same as UMAX Astra 4700. A backend is currenly beeing developed.
iVina FB2400 | USB | unsupported | Not supported. No chipset information available. Same as UMAX Astra 6700.
Benq | 310p | Parport | unsupported | Unsupported. No details about the protocol known.
610p | Parport | unsupported | Unsupported. No details about the protocol known.
620p | Parport | unsupported | Unsupported. No details about the protocol known.
620pt | Parport | unsupported | Unsupported. No details about the protocol known.
Boeder | Sm@rtScan Office | Parport USB | unsupported | Unsupported. Vendor/product 0x5cb, 0x1483. According to linux-usb.org that's the same ids as Trust Trust CombiScan 19200. The vendor is PowerVision Technologies, Inc. Maybe also a PV8630 as in the UMAX 1200U?
Brother | DCP 8020 | USB | unsupported | Unsupported. See link for details.
MFC 4600 | Parport USB | unsupported | Unsupported. However there is a project to support this scanner/printer/fax combination. See link.
MFC 5100c | Parport USB | unsupported | Unsupported. Some information is available (see link). See also MFC 4600.
MFC 6800 | USB | unsupported | Unsupported. A backend is under development (see link). Vendor/product 0x04f9/0x0111. See also MFC 4600.
MFC 9160 | USB Parport | unsupported | Unsupported. Maybe it's similar to the other Brother MFCs?
Canon | CanoScan 3000 | USB | unsupported | Probably unsupported. See link.
CanoScan 3000F | USB | unsupported | Probably unsupported. See link.
CanoScan 5000F | USB | unsupported | Probably unsupported. See link for details.
CanoScan 8000F | USB | unsupported | Not supported. USB Vendor/product 0x04a9/0x220f. See link for more information. With transparency adapter.
CanoScan 9900F | USB | unsupported | Probably unsupported, similar to 8000F. Vendor/product 0x04a9/0x2210. 3200x6400 dpi USB2. With transparency adapter.
CanoScan D646U | USB | unsupported | Probably not supported. USB Vendor/product 0x04a9/0x220b. See link for more information and test program.
CanoScan D660U | USB | unsupported | Unsupported. Vendor/product 0x04a9/0x2208. See link for more information.
CanoScan D1250U2 | USB | unsupported | Not supported. However, someone started working on this scanner and some information is available (see link).
CanoScan D2400UF | USB | unsupported | Not supported. See link.
CanoScan FB620U | USB | unsupported | Probably not supported. Vendor/product 0x4a9/0x2202. Some information is available.
CanoScan FB1210U | USB | unsupported | Not supported. Vendor/product 0x4a9/0x2205. However, a stand-alone program for FreeBSD is available.
DR-2080C | USB SCSI | unsupported | Probably not supported. Path-trough (ADF) scanner.
FS4000 | USB SCSI | unsupported | Not supported. USB Vendor/product 0x04a9/0x3042. See link for more details.
IS 12 | USB | unsupported | Probably not supported. This scanner is used in a number of Canon portable printers (BJC-80 for one). No further information available.
CanoScan LiDE 50 | USB | unsupported | Probably not supported yet. Some information is available.
CanoScan LiDE 80 | USB | unsupported | Probably not supported yet. Some information is available.
Compaq | S200 | USB | unsupported | Not supported. 2400x1200 dpi. Vendor=0x049f, Product=0x0021. One bulk-in, one bulk-out and one interrupt endpoint. Type-number: U0001-HB21, another type nr on the inside: 75100512-00
S4 100 | USB | unsupported | Not supported. Vendor=0x049f, Product=0x001a.
Corex | Cardscan 500 | USB | unsupported | Probably not supported. Businesscard reader. Vendor/product: 0x08f0/0x0001.
Epson | Perfection 3170 | USB | unsupported | Probably unsupported. Support is planned by the (external) epkowa backend. Seems to neither use Epson nor Benq protocol. Details appreciated.
E-Lux | j-6121 | Parport | unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121.
Enhans | j-6121 | Parport | unsupported | Probably unsupported. Sold 1998. Same as E-Lux j-6121.
M-3630 A | Parport | unsupported | Probably unsupported.
Fujitsu | fi-4010C | USB | unsupported | Unsupported. Vendor/product: 0x04c5, 0x1029. Maybe similar to fi-4220C?
fi-4110CU | USB | unsupported | Unsupported. Vendor/product unknown. Maybe similar to fi-4220C?
Genius | ColorPage HR6X Slim | USB | unsupported | Not supported. Vendor/product: 0x0458/0x2019. GL646. See link for more details.
ColorPage HR7X Slim | USB | unsupported | Not supported. Vendor/product: 0x0458/0x2018. GL646. See link for more details.
ColorPage HR8 | USB | unsupported | Not supported. See link for some more details.
Colorpage Vivid III | USB | unsupported | Not supported. Vendor/product: 0x07b3/0x0001. See link for details.
Hewlett-Packard | Photo Scanner 1000 | USB | unsupported | Not supported by SANE. However, it's detected as mass storage device so just mounting it is reported to work. See link for devices data.
Photosmart 1200 Photo | USB | unsupported | Probably not supported by SANE. No details known. 10x15 cm. Maybe similar to Photo Scanner 1000?
ScanJet 2300C | USB | unsupported | Unsupported. See link for details.
ScanJet 2400C | USB | unsupported | Probably unsupported. See link for details.
ScanJet 3500c | USB | unsupported | Unsupported. Seems to use RealTek RTS8801C2-6. Vendor/Product ID 0x03F0/0x2205. See link and other Scanjet 35x0c entries.
ScanJet 3530c | USB | unsupported | Unsupported. Chipset is Realtek RTS8801C2-6. Vendor/Product ID 0x03F0/0x2005. See link and other Scanjet 35x0c entries.
ScanJet 3570c | USB | unsupported | Unsupported. Probably Realtek RTS8801C2-6, same ids as Scanjet 3530c. Has a TA. Vendor/product id 0x03F0/0x2005. See link and other Scanjet 35x0c entries.
ScanJet 3570cxi | USB | unsupported | Unsupported. See 3570c.
ScanJet 3670c | USB | unsupported | Probably unsupported. See link for more details.
ScanJet 3970c | USB | unsupported | Unsupported. See link for details.
ScanJet 4500C | USB | unsupported | Not supported. Landscape scanner. Same as 5500C, but without ADF. Same ID as 5550c.
ScanJet 4570C | USB | unsupported | Not supported. See link for details.
ScanJet 5500C | USB | unsupported | Not supported. See link for details.
ScanJet 5550C | USB | unsupported | Not supported. Same as 4570C, but with ADF. See link for details.
ScanJet 8200C | USB | unsupported | Not supported. SCSI optional. Includes TA. No further information.
ScanJet 8250C | USB | unsupported | Not supported. SCSI optional. Includes ADF and TA. Probably similar to 8200C. No further information.
ScanJet 8290C | USB | unsupported | Not supported. SCSI optional. Includes ADF and TA. Similar to 8200C? No further information.
IBM | ADF Color Scanner | Proprietary | unsupported | Unsupported. Uses proprietary ISA card. Maybe the same as the Plustek Spectra ADF?
Lexmark | X75 | USB | unsupported | Unsupported. See link for details.
X83 | USB | unsupported | Unsupported. Vendor/product 0x043d/0x003d. GL640.
Medion/Lifetec/Tevion/Cytron | MD 5345 | USB | unsupported | Probably unsupported. Vendor/product 0x0461/0x0377. See link for details.
MD 6228 | USB | unsupported | Probably unsupported. Vendor/product 0x0461/0x0377. See link for details.
Memorex | 6136u | USB | unsupported | Probably unsupported.
6142u | USB | unsupported | Probably unsupported. Same as Visioneer Onetouch 4400. See link for details.
Microtek | ScanMaker 336 CX | SCSI | unsupported | Probably unsupported. Seems to be similar to the Microtek 330 CX and is detected by the microtek2 backend. Scanning doesn't seem to work however.
ScanMaker 3630 | USB | unsupported | Unsupported. Doesn't seem to be compatible to 3600 series, see link.
ScanMaker 3800 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 3830 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 3840 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 4800 | USB | unsupported | Unsupported. Vendor/Product ids: 0x05da/0x30cf. SQ Scan08? See link for more details.
ScanMaker 4900 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 5600 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 5900 | USB | unsupported | Unsupported. See link for more details.
ScanMaker 6700 | USB IEEE-1394 | unsupported | Unsupported. See link.
ScanMaker 9600XL | USB SCSI IEEE-1394 | unsupported | Probably unsupported.
ScanMaker 9800XL | USB SCSI IEEE-1394 | unsupported | Unsupported. See link.
ScanPort 3000 | USB | unsupported | Unsupported. Vendor/Product ids: 0x04a7/0x0224. Realtek RTS8801B?. See link for details.
Minolta | Dual Scan III | USB | unsupported | Unsupported. May work with vuescan. See link for details.
DiMAGE Scan Elite 5400 | USB IEEE-1394 | unsupported | Probably unsupported. May work with vuescan. See link for details.
Mustek | 1800 A3 Pro-1 | USB | unsupported | Not supported but someone wants to start writing a backend. See link. Vendor/Product ids: 0x055f/0x0401. No information about this scanner on any Mustek website.
2400 M | USB | unsupported | Probably unsupported. No details known.
BearPaw 1248CU | USB | unsupported | Probably unsupported. No details known.
BearPaw 2400 TA Pro | USB | unsupported | Not supported. See link for some information.
BearPaw 2448 TA Pro | USB | unsupported | Not supported. See link for some information.
BearPaw 4800 TA Pro | USB | unsupported | Not supported. See link for some information.
P 3600 A3 Pro | USB | unsupported | Not supported. Maybe similar to the 1800 A3 Pro-1?. See link.
Paragon 600 II ED/EP | Parport | unsupported | Not supported by SANE yet, but there is a stand-alone program and support will be added to the mustek backend.
ScanExpress 600 USB | USB | unsupported | Unsupported. Vendor/Product 0x055f/0x873. Programming information is available.
ScanExpress 1200 USB | USB | unsupported | Unsupported. Vendor/Product 0x055f/0x0003. Programming information is available.
ScanExpress 1200 USB Plus | USB | unsupported | Unsupported. Vendor/Product 0x055f/0x0007.
ScanExpress 12000 P | Parport | unsupported | Not supported. Asic 1505/05.
ScanExpress CardSmart | USB | unsupported | Probably unsupported. USB business card scanner. Maybe works as USB storage device?
ScanMagic 9636P | Parport | unsupported | Probably not supported. Same as Mustek 12000 P?. ASIC 1505.
Optrox | PhotoMaker 3 | Parport | unsupported | Probably not supported.
Pentax | DSmobile USB | USB | unsupported | Probably not supported. Some information is available.
PIE | Primefilm 1800u | USB | unsupported | Not supported. Vendor/product 0x05e3/0x0120. See link for details.
Powerslide 3600 | USB IEEE-1394 | unsupported | Probably unsupported. Film scanner that can scan directly from the magazine.
Packard Bell | Diamond 1200 | USB | unsupported | Probably not supported yet. No information available. If you own such a device, please contact us.
Plustek | OpticPro 1212U | USB | unsupported | Vendor/product: 0x07b3/0x0001. Same ids as early U12/UT12 models, maybe the same chip?
OpticPro A3U | USB | unsupported | Uses Plustek ASIC P99002
OpticPro S6 | USB | unsupported | Uses RealTek chipset (RTL8801D)
OpticPro S12 | USB | unsupported | Uses the Genesys Logic GL646 chipset.
OpticPro ST12 | USB | unsupported | Uses the Genesys Logic GL646 chipset.
OpticPro S24 | USB | unsupported | Not supported yet. May be supported later, see link for details.
OpticPro ST24 | USB | unsupported | Not supported yet. May be supported later, see link for details.
OpticPro U12/UT12 | USB | unsupported | All devices using product ID 0x0001 are not supported, for others see Plustek backend. The older models seem to use a P98003 parallel port ASIC and a GenesysLogic parport-over USB brigde. The P98003 is also used by the P12 and PT12 models.
OpticPro S28 | USB | unsupported | Uses Plustek ASIC.
OpticPro S48 | USB | unsupported | Uses Plustek ASIC.
OpticSlim 2400 | USB | unsupported | Probably the same as OpticSlim 1200, with higher resolution.
Spectra ADF | Proprietary | unsupported | Unsupported. Uses proprietary ISA card that also provides power and is labelled GPS-1 PAGE-A from Taiwan. Other labels on the scanner include ADF Color Scanner and SF600AS. Maybe the same as the IBM ADF Color Scanner?
Primax | Colorado 600U | USB | unsupported | Not supported. Some information is available.
Colorado 2400U | USB | unsupported | Probably unsupported. ASIC EICI 10440A. Vendor/product 0x461/0x346. May work with viceo backend(?), see link.
Primascan Colorado 2600u | USB | unsupported | Unsupported. Same as Visioneer Onetouch 4400. See link for details.
Colorado Direct 600 | Parport | unsupported | Not supported. However, a stand-alone program is available.
Colorado Direct 9600 | Parport | unsupported | Not supported. However, a stand-alone program is available.
Slim-Line 1200 | USB | unsupported | Probably unsupported. Vendor/product maybe 0x0461/0x0377. Maybe the same as Medion MD 6228/MD 5345
Prolink | Winscan Pro 2448U | USB | unsupported | Not supported. Some information is available. Vendor=0x06dc product=0x0014. RealTek RTS8801.
Reflecta | DigitDia 3600 | USB IEEE-1394 | unsupported | Probably unsupported. Film scanner that can scan directly from the magazine.
iScan 1800 | USB | unsupported | Probably unsupported. See link for details.
Relisys | Scorpio Ultra 3 | USB | unsupported | Probably unsupported. See link for details.
Sicos | DMS 2000 | proprietary | unsupported | Not supported until now. Work on a backend has started, contact the author for details (see link)
Spot Technology | Maxiscan A4 | proprietary | unsupported | Not supported until now. Work on a backend has started, see link for more information.
ScanTak 2c | proprietary | unsupported | Not supported. Work on a backend has started, see link for more information.
ScanTak 3c | proprietary | unsupported | Not supported. Work on a backend has started, see link for more information.
Syscan | TravelScan 460/464 | USB | unsupported | Not supported. Some information is available. May work with the Plustek backend in future.
TravelScan Pro | USB | unsupported | Probably not supported. Some information is available.
TCE | MK600U | USB | unsupported | Not supported. Some information is available.
Trust | CombiScan 19200 | Parport USB | unsupported | Unsupported. Vendor/product 0x5cb, 0x1483 according to linux-usb.org. Same ids as Boeder Sm@rtScan Office. The vendor is PowerVision Technologies, Inc. Maybe also a PV8630 as in the UMAX 1200U?
UMAX | Astra 2100 U | USB | unsupported | Probably not supported. See link for details.
Astra 3600 | USB | unsupported | Probably not supported. See link for details.
Astra 4400 | USB | unsupported | Probably not supported. See link for details.
Astra 4450 | USB | unsupported | Probably not supported. See link for details.
Astra 4500 | USB | unsupported | Not supported. Vendor/product 0x0638/0x0a10. GL646. Same as Avision iVina FB1600. A backend is currenly beeing developed. See link for more details.
Astra 4700 | USB | unsupported | Not supported. GL660 + GL646. Same as Avision iVina FB1800. A backend is currenly beeing developed. See link for more details.
Astra 6700 | USB | unsupported | Not supported. No chipset information available. Same as Avision iVina FB2400.
AstraSlim 1200 SE | USB | unsupported | Probably not supported currently. May be supported in future. See link for more details.
Powerlook 1000 USB | USB | unsupported | Probably not supported. No further information available.
Visioneer | 6200 | USB | unsupported | Not supported. Is reported to use the E5 chipset. Uses a Primax ID. See link for some details. Looks similar to Primascan Colorado 2600u.
Onetouch 4400 | USB | unsupported | Not supported. E5 chipset? Vendor/product 0x0461/0x0347.See link for more details.
OneTouch 4800 USB | USB | unsupported | Unsupported. Vendor/Product ids: 0x04a7/0x0224. Seems to use Realtek RTS8801B. Same as Microtek Scanport 3000. See link for details.
OneTouch 5300 USB | USB | unsupported | Not supported. Vendor/product ids 0x04a7/0x0226. Chipset is RTS8801B(?). See link for output of /proc/bus/usb/devices.
OneTouch 5800 USB | USB | unsupported | Unsupported. 48 bit scanner, doesn't work with viceo backend. RTS8801C. Vendor/product 0x04a7/0x0226.
OneTouch 7100 | USB | unsupported | Unsupported. See link for details.
Onetouch 8700 | USB | unsupported | Not supported. Same as 8920 but without TA?
Onetouch 8900 | USB | unsupported | Not supported. Same as 8920 but without TA?
Onetouch 8920 | USB | unsupported | Not supported. Same as 8700 and 8900 but includes a TA. Uses a Primax ID. Chipset is RTS8801C. See link for output of /proc/bus/usb/devices.
Onetouch 9020 | USB | unsupported | Not supported. Vendor/product: 0x04a7/0x022c.
PaperPort 3100b | Parport | unsupported | Most probably not supported. More details would be appreciated.
Primascan Colorado 2600u | USB | unsupported | Not supported. See Visioneer Onetouch 4400.
Xerox | WorkCentre XK35c | USB Parport | unsupported | Not supported. See link for more details.
WorkCentre Pro 412 | USB Parport | unsupported | Not supported. See link for more details.

## Still Cameras

Backends: dc25, dc210, dc240, dmc

### Backend: dc25 (1.2)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-dc25

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Kodak | DC25 | Serial port | complete |
DC20 | Serial port | basic | DC-20 untested by author but reported to work

### Backend: dc210 (0.0)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-dc210

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Kodak | DC210 | Serial port | basic |

### Backend: dc240 (0.0)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-dc240

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Kodak | DC240 | Serial port | good | Use gphoto2 backend to get USB support

### Backend: dmc (unmaintained)

Manual page: sane-dmc

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Polaroid | DMC | SCSI | good |

## Video Cameras

Backends: qcam

### Backend: qcam (unmaintained)

Manual page: sane-qcam

Manufacturer | Model | Interface | Status | Comment
--- | --- | --- | --- | ---
Connectix | Color QuickCam | Parport | good | Requires root privileges.
Greyscale QuickCam | Parport | minimal | Requires root privileges. Partly working.

## APIs

Backends: gphoto2, pint, pnm, test, v4l

### Backend: gphoto2 (0.0)

Link(s): mailto:peter@fales-lorenz.net
Manual page: sane-gphoto2
Description: Multiple cameras supported by the gphoto2 libraries
Comment: The long-term plan is to support all the cameras supported by the gphoto2 libraries (currently over 140 models). However, at this stage, only a handful of cameras are definitely known to work with SANE. Other cameras will probably work if the native file format is EXIF or JPEG. Testers welcome!

### Backend: pint (unmaintained)

Manual page: sane-pint
Description: Scanners with the machine-independent PINT interface
Comment: Haven't been tested for a long time. Handle with care.

### Backend: pnm (1.0.8)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-pnm
Description: Reads PNM files
Comment: Used for debugging frontends. Obsolete, use test backend instead.

### Backend: test (1.0-25)

Link(s): http://www.meier-geinitz.de/sane/test-backend/
Manual page: sane-test
Description: Frontend-tester
Comment: Backend for testing frontends. Also serves as example for SANE backend options.

### Backend: v4l (1.0-2)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-v4l
Description: Interface to Video For Linux API
Comment: Supports video cameras and other devices accessed by the v4l kernel API, e.g. bttv devices. Quite a lot of known bugs.

## Meta Backends

Backends: dll, net

### Backend: dll (1.0.8)

Link(s): mailto:henning@meier-geinitz.de
Manual page: sane-dll
Description: Dynamic loading of shared-library backends.

### Backend: net (1.0.12)

Link(s): http://www.penguin-breeder.org/?page=sane-net
Manual page: sane-net
Description: Network access to saned servers
Comment: Can be used to access any scanner supported by SANE over the net. Supports IPv4 and IPv6.

### Legend:

> Backend:
>   Name of the backend, in parentheses if available: Version of backend/driver; newer versions may be available from their home sites.
>   NEW! means brand-new to the current release of SANE.
>   UNMAINTAINED means that nobody maintains that backend. Expect no new features or newly supported devices. You are welcome to take over maintainership.
> Link(s):
>   Link(s) to more extensive and detailed information, if it exists, or the email address of the author or maintainer.
> Manual Page:
>   A link to the man-page online, if it exists.
> Comment:
>   More information about the backend or model, e.g. the level of support and possible problems.
> Manufacturer:
>   Manufacturer, vendor or brand name of the device.
> Model:
>   Name of the the device.
> Interface:
>   How the device is connected to the computer.
> Status:
>   Indicates how many of the features the device provides are supported by SANE.
>   - unsupported means the device is not supported at least by this backend. It may be supported by other backends, however.
>   - untested means the device may be supported but couldn't be tested. Be very careful and report success/failure.
>   - minimal means that the device is detected and scans at least in one mode. But the quality is bad or important features won't work.
>   - basic means it works at least in the most important modes but quality is not perfect.
>   - good means the device is usable for day-to-day work. Some rather exotic features may be missing.
>   - complete means the backends supports everything the device can do.
> Description:
>   The scope of application of the backend.

SANE homepage
This page was last updated on Sun Nov 23 01:26:34 2003