# Scanner information
Author: Henning Meier-Geinitz
Keywords: sane, backend, driver, scanner, unsupported

# Scanners not supported by SANE

## Manufacturer and model

Genius ColorPage HR7X

## Bus type

USB

## Vendor ID

0x0458

## Product ID

0x2018

## Chipset

Is reported to use the GL646 chipset

## Comments

May be supported by the Genesys backend, when it's finished.

## Output of /proc/bus/usb/devices or sane-find-scanner -v -v

    T:  Bus=03 Lev=01 Prnt=01 Port=01 Cnt=01 Dev#=  2 Spd=12  MxCh= 0
    D:  Ver= 1.10 Cls=00(>ifc ) Sub=00 Prot=00 MxPS= 8 #Cfgs=  1
    P:  Vendor=0458 ProdID=2018 Rev= 0.00
    S:  Manufacturer=KY
    S:  Product=CP-HR7X Slim
    C:* #Ifs= 1 Cfg#= 1 Atr=e0 MxPwr= 48mA
    I:  If#= 0 Alt= 0 #EPs= 3 Cls=10(unk. ) Sub=01 Prot=00 Driver=usbscanner
    E:  Ad=81(I) Atr=02(Bulk) MxPS=  64 Ivl=0ms
    E:  Ad=02(O) Atr=02(Bulk) MxPS=  64 Ivl=0ms
    E:  Ad=83(I) Atr=03(Int.) MxPS=   1 Ivl=8ms

    <device descriptor of 0x0458/0x2018 at 001:002 (KY CP-HR7X Slim)>
    bLength               18
    bDescriptorType       1
    bcdUSB                1.10
    bDeviceClass          0
    bDeviceSubClass       0
    bDeviceProtocol       0
    bMaxPacketSize0       8
    idVendor              0x0458
    idProduct             0x2018
    bcdDevice             0.00
    iManufacturer         10 (KY)
    iProduct              11 (CP-HR7X Slim)
    iSerialNumber         0 ()
    bNumConfigurations    1
     <configuration 0>
     bLength              9
     bDescriptorType      2
     wTotalLength         39
     bNumInterfaces       1
     bConfigurationValue  1
     iConfiguration       0 ()
     bmAttributes         224 (Self-poweredRemote Wakeup)
     MaxPower             48 mA
      <interface 0>
       <altsetting 0>
       bLength            9
       bDescriptorType    4
       bInterfaceNumber   0
       bAlternateSetting  0
       bNumEndpoints      3
       bInterfaceClass    16
       bInterfaceSubClass 1
       bInterfaceProtocol 0
       iInterface         0 ()
        <endpoint 0>
        bLength           7
        bDescriptorType   5
        bEndpointAddress  0x81 (in 0x01)
        bmAttributes      2 (bulk)
        wMaxPacketSize    64
        bInterval         0 ms
        bRefresh          0
        bSynchAddress     0
        <endpoint 1>
        bLength           7
        bDescriptorType   5
        bEndpointAddress  0x02 (out 0x02)
        bmAttributes      2 (bulk)
        wMaxPacketSize    64
        bInterval         0 ms
        bRefresh          0
        bSynchAddress     0
        <endpoint 2>
        bLength           7
        bDescriptorType   5
        bEndpointAddress  0x83 (in 0x03)
        bmAttributes      3 (interrupt)
        wMaxPacketSize    1
        bInterval         8 ms
        bRefresh          0
        bSynchAddress     0
    found USB scanner (vendor=0x0458 [KY], product=0x2018 [CP-HR7X Slim]) at libusb:001:002

# Want to add or correct information?

If anything is wrong or missing on this page please file a bug report or use the the form for adding an unsupported device.

If you own an unsupported scanner, please send as much information as possible. Especially the output of sane-find-scanner -v -v and/or cat /proc/scsi/scsi (for SCSI scanners) or cat /proc/bus/usb/devices (for USB scanners) can help. If you dare to open the scanner, have a look at the text that's printed on the chips. That may help to identify the chipset. If you know that the scanner is similar to another one (e.g. supported by the same Windows driver), please also mention this fact.

# Information for Manufacturers

Are you a manufacturer or vendor of scanners and one of your scanners is not supported by SANE yet? In this case please have a look at our information for manufacturers.

# Links

- General information on how to contribute to SANE, e.g. by writing backends
- Scanner search engine
- SANE homepage

SANE homepage
Contact

$Date$ $Author$