The Status page provides an overview of your Stratux device.

The current state of you device is shown at th top - `Connected` in green or `Disconected`in red.

Depending on the hardware you have installed in your Stratux, you will have status for the following:

- SDR (software defined radio) dongle tuned to 978 MHz for UAT (universal access transceiver) traffic and weather
- SDR (software defined radio) dongle tuned to 1090 MHz for ES (extended squitter) traffic
- GPS the RY835AI module receiving GPS data from satellites
- AHRS the RY835AI module generating attitude data from its pressure sensor, gyroscope, accelerometer, and magnetometer.

NOTE: This page only shows devices you have installed and turned on (via the Settings page.

The Messages section gives you details for messages received. There are statistics for the rolling average for the past 60 seconds as well as the peak average.

For GPS and AHRS you can view the number of satellites being received and if AHRS is configured and operating.

The Status page also gives you an indication of how long your Stratux devices has been operating since you turned it on, as well as reporting the on-board temperature sensor of the Raspberry Pi.