<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.2">
<drawing>
<library>
<packages>
<package name="TTGO-T-DISPLAY-OL">
</package>
<package name="TTGO-T-DISPLAY-OP">
</package>
</packages>
<symbols>
<symbol name="TTGO-T-DISPLAY">
<pin name="GND" direction="pwr"/>
<pin name="3V3" direction="pwr"/>
<pin name="5V" direction="pwr"/>
<pin name="2/A12"/>
<pin name="15/A13"/>
<pin name="13/A14"/>
<pin name="12/A15" direction="out"/>
<pin name="21/SDA"/>
<pin name="22/SCL"/>
<pin name="26/A19/DAC2"/>
<pin name="25/A18/DAC1"/>
<pin name="39/A3/SVN"/>
<pin name="36/A0/SVP"/>
<pin name="37"/>
<pin name="38"/>
<pin name="32/A4"/>
<pin name="33/A5"/>
<pin name="27/A17"/>
<pin name="17"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TTGO-T-DISPLAY">
<description>TTGO-TDisplay
https://github.com/Xinyuan-LilyGO/TTGO-T-Display</description>
<gates>
<gate name="G$1" symbol="TTGO-T-DISPLAY"/>
</gates>
<devices>
<device name="FRAME" package="TTGO-T-DISPLAY-OL">
<connects>
<connect gate="G$1" pin="12/A15" pad="12-G12-A15"/>
<connect gate="G$1" pin="13/A14" pad="13-G13-A14"/>
<connect gate="G$1" pin="15/A13" pad="15-G15-A13"/>
<connect gate="G$1" pin="17" pad="17-DIONLY"/>
<connect gate="G$1" pin="2/A12" pad="2-G2-A12"/>
<connect gate="G$1" pin="21/SDA" pad="21-SDA"/>
<connect gate="G$1" pin="22/SCL" pad="22-SCL"/>
<connect gate="G$1" pin="25/A18/DAC1" pad="25-G25-A18-DAC1"/>
<connect gate="G$1" pin="26/A19/DAC2" pad="26-G26-A19-DAC2"/>
<connect gate="G$1" pin="27/A17" pad="27-G27-A17"/>
<connect gate="G$1" pin="32/A4" pad="32-G32-A4"/>
<connect gate="G$1" pin="33/A5" pad="33-G33-A5"/>
<connect gate="G$1" pin="36/A0/SVP" pad="SVP-G36-A0"/>
<connect gate="G$1" pin="37" pad="37-G37"/>
<connect gate="G$1" pin="38" pad="38-G38"/>
<connect gate="G$1" pin="39/A3/SVN" pad="SVN-G39-A3"/>
<connect gate="G$1" pin="3V3" pad="3V3_0 3V3_1"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="GND" pad="GND_0 GND_1 GND_2 GND_3 GND_4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PINS" package="TTGO-T-DISPLAY-OP">
<connects>
<connect gate="G$1" pin="12/A15" pad="12-G12-A15"/>
<connect gate="G$1" pin="13/A14" pad="13-G13-A14"/>
<connect gate="G$1" pin="15/A13" pad="15-G15-A13"/>
<connect gate="G$1" pin="17" pad="17-NA"/>
<connect gate="G$1" pin="2/A12" pad="2-G2-A12"/>
<connect gate="G$1" pin="21/SDA" pad="21-SDA"/>
<connect gate="G$1" pin="22/SCL" pad="22-SCL"/>
<connect gate="G$1" pin="25/A18/DAC1" pad="25-G25-A18-DAC1"/>
<connect gate="G$1" pin="26/A19/DAC2" pad="26-G26-A19-DAC2"/>
<connect gate="G$1" pin="27/A17" pad="27-G27-A17"/>
<connect gate="G$1" pin="32/A4" pad="32-G32-A4"/>
<connect gate="G$1" pin="33/A5" pad="33-G33-A5"/>
<connect gate="G$1" pin="36/A0/SVP" pad="SVP-G36-A0"/>
<connect gate="G$1" pin="37" pad="37-G37"/>
<connect gate="G$1" pin="38" pad="38-G38"/>
<connect gate="G$1" pin="39/A3/SVN" pad="SVN-G39-A3"/>
<connect gate="G$1" pin="3V3" pad="3V3_0 3V3_1"/>
<connect gate="G$1" pin="5V" pad="5V"/>
<connect gate="G$1" pin="GND" pad="GND_0 GND_1 GND_2 GND_3 GND_4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
