# f055:9800, 9801, 9802 MicroPython pyboard 
# Instantiate Pyboard V1.0, V1.1 or Lite as /dev/pyoard
ATTRS{idVendor}=="f055", ENV{MTP_NO_PROBE}="1"
ATTRS{idVendor}=="f055", ENV{ID_MM_DEVICE_IGNORE}="1" 
SUBSYSTEMS=="usb", ATTRS{idVendor}=="f055", MODE:="0666"
KERNEL=="ttyACM*", ATTRS{idVendor}=="f055", SYMLINK+="pyboard", MODE:="0666"
KERNEL=="ttyUSB*", ATTRS{idVendor}=="f055", SYMLINK+="pyboard", MODE:="0666"
# DFU mode
SUBSYSTEMS=="usb", ATTRS{idVendor}=="0483", ATTRS{idProduct}=="df11", MODE:="0666"
