# Scanner information
Author: Henning Meier-Geinitz
Keywords: sane, backend, driver, scanner, unsupported

# Scanners not supported by SANE

## Manufacturer and model

Mustek Paragon 600 II EP
Mustek Paragon 600 II ED

## Bus type

Parport

## Vendor ID

--

## Product ID

--

## Chipset

SCSI over parport

## Comments

There is no SANE backend yet, but a scan program for the 600 II EP. Please report if it also works for the 600 II ED. Some information is also in the sane-devel posts (another one).

This is a SCSI-over-parallel-port scanner. It will be supported by the SANE Mustek backend in future, work is currently done for that goal. There is more information on this scanner on sane-devel, search the archives for August, 2003.

## Output of /proc/bus/usb/devices or sane-find-scanner -v -v

    --

# Want to add or correct information?

If anything is wrong or missing on this page please file a bug report or use the the form for adding an unsupported device.

If you own an unsupported scanner, please send as much information as possible. Especially the output of sane-find-scanner -v -v and/or cat /proc/scsi/scsi (for SCSI scanners) or cat /proc/bus/usb/devices (for USB scanners) can help. If you dare to open the scanner, have a look at the text that's printed on the chips. That may help to identify the chipset. If you know that the scanner is similar to another one (e.g. supported by the same Windows driver), please also mention this fact.

# Information for Manufacturers

Are you a manufacturer or vendor of scanners and one of your scanners is not supported by SANE yet? In this case please have a look at our information for manufacturers.

# Links

- General information on how to contribute to SANE, e.g. by writing backends
- Scanner search engine
- SANE homepage

SANE homepage
Contact

$Date$ $Author$